{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPVX10A4V / EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPVX10S18AJ4V / EPSK08ARW1","EPVX10S23AJ4V / EPSK08ARW1","EPVX10S18AJ4V / EPSK10ARW1","EPVX10S23AJ4V / EPSK10ARW1"]
["Indoor unit","","","","","EPVX10S18AJ4V","EPVX10S23AJ4V","EPVX10S18AJ4V","EPVX10S23AJ4V"]
["Heating capacity","Nom.","","","kW","7.62 (1)","7.62 (1)","8.11 (1)","8.11 (1)"]
["Cooling capacity","Nom.","","","kW","6.89 (3), 6.37 (4)","6.89 (3), 6.37 (4)","7.84 (3), 6.37 (4)","7.84 (3), 6.37 (4)"]
["Power input","Heating","","Nom.","kW","1.52 (1)","1.52 (1)","1.64 (1)","1.64 (1)"]
["","Cooling","","Nom.","kW","1.85 (3), 1.13 (4)","1.85 (3), 1.13 (4)","2.17 (3), 1.13 (4)","2.17 (3), 1.13 (4)"]
["","Domestic hot water from 10°C to 50°C","","Nom.","kWh","2.35","2.89","2.35","2.89"]
["Heat up time from 10°C to 50°C","hr","","","","1h 27min","1h 58min","1h 27min","1h 58min"]
["COP","","","","","5.01 (1)","5.01 (1)","4.94 (1)","4.94 (1)"]
["EER","","","","","3.73 (3), 5.63 (4)","3.73 (3), 5.63 (4)","3.62 (3), 5.63 (4)","3.62 (3), 5.63 (4)"]
["Domestic hot water heating","General","","Declared load profile","","L","L","L","L"]
["","Average climate","","Water heating energy efficiency class","","A+","A+","A+","A+"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.94","3.94","3.99","3.99"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["","Average climate water outlet 35°C","General","SCOP","","5.14","5.14","5.14","5.14"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB","(2) - Cooling: EW 12°C; LW 7°C; ambient conditions: 35°CDB"]
["","","","","","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB","(3) - Cooling: EW 23°C; LW 18°C; ambient conditions: 35°CDB"]