{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DV"]
[]
[]
[]
[]
["","","","","","ERLA03DAV3"]
["Dimensions","Unit","","Height","mm","550"]
["","","","Width","mm","765"]
["","","","Depth","mm","285"]
["Weight","Unit","","","kg","35"]
["Fan","Air flow rate","Heating","High","m³/min","32.0"]
["","","Cooling","High","m³/min","36"]
["Operation range","Cooling","","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["","Domestic hot water","","Min.","°CDB","-15"]
["","","","Max.","°CDB","35"]
["Sound power level","Heating","","Nom.","dBA","59"]
["","Cooling","","Nom.","dBA","60"]
["Sound pressure level","Heating","","Nom.","dBA","46"]
["","Cooling","","Nom.","dBA","46"]
["Refrigerant","Type","","","","R-32"]
["","GWP","","","","675.0"]
["","Charge","","","tCO2Eq","0.675"]
["","Charge","","","kg","1"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.52"]
["","Level difference","IU - OU","Max.","m","20.0"]
["Power supply","Name","","","","V3"]
["","Phase","","","","1N~"]
["","Power supply-=-Frequency","","Frequency","","50"]
["","Power supply-=-Voltage","","Voltage","","220-240"]
["Current","Current-=-Recommended fuses","","Recommended fuses","","16"]
["Notes","","","","","(1) - Cooling Ta 35°C - LWE 18°C (DT = 5°C); Heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]