{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":17,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWLQ-L-SS"]
[]
[]
[]
[]
["","","","","EWLQ180L-SS","EWLQ205L-SS","EWLQ230L-SS","EWLQ260L-SS","EWLQ290L-SS","EWLQ330L-SS","EWLQ380L-SS","EWLQ430L-SS","EWLQ480L-SS","EWLQ540L-SS","EWLQ600L-SS","EWLQ660L-SS","EWLQ720L-SS"]
["Sound pressure level","Cooling","Nom.","dBA","65 (2)","68 (2)","70 (2)","72 (2)","74 (2)","74 (2)","73 (2)","76 (2)","77 (2)","77 (2)","78 (2)","78 (2)","78 (2)"]
["Sound power level","Cooling","Nom.","dBA","83","86","88","90","91","91","91","93","95","95","95","96","96"]
["Refrigerant","Circuits","Quantity","","2","2","2","2","2","2","2","2","2","2","2","2","2"]
["","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Type","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Dimensions","Unit","Width","mm","928","928","928","928","928","928","928","928","928","928","928","928","928"]
["","","Depth","mm","2,801","2,801","2,801","2,801","2,801","2,801","2,801","2,801","2,801","2,801","2,801","2,801","2,801"]
["","","Height","mm","1,970","1,970","1,970","1,970","1,970","1,970","1,970","1,970","1,970","2,090","2,210","2,210","2,210"]
["Compressor","Type","","","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor"]
["","Quantity","","","4","4","4","4","4","4","4","4","4","4","4","4","4"]
["Capacity control","Minimum capacity","","%","25.0","21.0","25.0","22.0","25.0","23.0","25.0","21.0","25.0","22.0","20.0","18.0","25.0"]
["","Method","","","Step","Step","Step","Step","Step","Step","Step","Step","Step","Step","Step","Step","Step"]
["Weight","Operation weight","","kg","894","1,081","1,292","1,345","1,436","1,486","1,547","1,638","1,690","1,741","1,844","1,990","2,120"]
["","Unit","","kg","832","1,007","1,202","1,252","1,333","1,380","1,432","1,511","1,560","1,609","1,694","1,833","1,957"]
["Water heat exchanger - evaporator","Type","","","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger","Plate heat exchanger"]
["Cooling capacity","Nom.","","kW","173 (1)","197 (1)","224 (1)","249 (1)","279 (1)","317 (1)","361 (1)","409 (1)","459 (1)","511 (1)","571 (1)","624 (1)","676 (1)"]
["EER","","","","3.91 (1)","3.86 (1)","3.87 (1)","3.79 (1)","3.81 (1)","3.78 (1)","3.86 (1)","3.79 (1)","3.84 (1)","3.78 (1)","3.76 (1)","3.71 (1)","3.67 (1)"]
["Piping connections","Discharge line connection","","inch","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 1\"5/8","1\"5/8 + 2\"1/8","2\"1/8 + 2\"1/8","2\"1/8 + 2\"1/8","2\"1/8 + 2\"1/8"]
["Power input","Cooling","Nom.","kW","44.3 (1)","51.1 (1)","57.9 (1)","65.6 (1)","73.2 (1)","83.8 (1)","93.5 (1)","108 (1)","119 (1)","135 (1)","152 (1)","168 (1)","184 (1)"]
["Power supply","Phase","","","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~","3~"]
["","Frequency","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Voltage","","V","400","400","400","400","400","400","400","400","400","400","400","400","400"]
["Notes","","","","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation.","(1) - Cooling: entering evaporator water temp. 12.0°C; leaving evaporator water temp. 7.0°C; condensing temperature 45.0°C, unit at full load operation."]
["","","","","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units","(2) - Sound power level (at standard conditions) is measured in accordance with ISO9614 and Eurovent 8/1 for Eurovent certified units"]
["","","","","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water","(3) - Fluid: Water"]
["","","","","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS).","(4) - For more details on the operating limits please refer to the Chiller Selection Software (CSS)."]
["","","","","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases","(5) - Its functioning relies on fluorinated greenhouse gases"]
["","","","","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%.","(6) - Allowed voltage tolerance ± 10%. Voltage unbalance between phases must be within ± 3%."]
["","","","","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load","(7) - Maximum starting current: starting current of biggest compressor + current of the other compressor at 75 % of maximum load"]
["","","","","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current","(8) - Nominal current cooling mode is referred to the following conditions: evaporator 12/7°C; condenser 30/35°C; compressors current"]
["","","","","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope","(9) - Maximum running current is based on max compressor absorbed current in its envelope"]
["","","","","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage.","(10) - Maximum unit current for wires sizing is based on minimum allowed voltage."]
["","","","","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1","(11) - Maximum current for wires sizing: compressor full load ampere x 1.1"]