{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWLT-Q-XSA"]
[]
[]
[]
[]
["","","","","","EWLT100Q-XSA1","EWLT125Q-XSA1","EWLT160Q-XSA1"]
["Cooling capacity","Nom.","","","kW","90.2","116.9","155"]
["Capacity control","Method","","","","Step","Step","Step"]
["","Minimum capacity","","","%","50","50","50"]
["Power input","Cooling","","Nom.","kW","23.67","31.1","38.55"]
["EER","","","","","3.81","3.76","4.02"]
["Dimensions","Unit","","Depth","mm","1300","1300","1300"]
["","","","Height","mm","1000","1000","1000"]
["","","","Width","mm","1200","1200","1200"]
["Weight","Operation weight","","","kg","382","428","482"]
["","Unit","","","kg","372","417","467"]
["Casing","Colour","","","","Ivory white","Ivory white","Ivory white"]
["","Material","","","","Galvanised steel","Galvanised steel","Galvanised steel"]
["Water heat exchanger - evaporator","Water pressure drop","Cooling","Nom.","kPa","17.16","17.93","19.55"]
["Compressor","Quantity","","","","2","2","2"]
["","Type","","","","Scroll","Scroll","Scroll"]
["Operation range","Water side","Evaporator","Min.","°CDB","-15","-15","-15"]
["","","","Max.","°CDB","30","30","30"]
["Sound power level","Cooling","","Nom.","dBA","80.99","84.19","85.99"]
["Sound pressure level","Cooling","","Nom.","dBA","65.4","68.6","70.4"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Charge","","","kg","0","0","0"]
["","Circuits","","Quantity","","1","1","1"]
["Piping connections","Evaporator water inlet/outlet (OD)","","","","3\"","3\"","3\""]
["Power supply","Phase","","","","3","3","3"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","400","400","400"]
["","Voltage range","","Min.","%","-10","-10","-10"]
["","","","Max.","%","+10","+10","+10"]
["Unit","Starting current","","Max","A","221","345","363"]
["","Running current","Cooling","Nom.","A","42.1","50","60.7"]
["","","","Max","A","62","80","97"]
["","Max unit current for wires sizing","","","A","68","88","107"]