{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":17,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYD-4ZXR"]
[]
[]
[]
[]
["","EWYD4004ZXRA2","EWYD4004ZXRB2","EWYD4504ZXRA2","EWYD4504ZXRB2","EWYD5004ZXRA2","EWYD5004ZXRB2","EWYD5504ZXRA2","EWYD5504ZXRB2","EWYD6004ZXRA2","EWYD6004ZXRB2","EWYD6504ZXRA2","EWYD6504ZXRB2","EWYD7004ZXRA2","EWYD7004ZXRB2","EWYD8004ZXRA2","EWYD8004ZXRB2"]
["Notes","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C.","(1) - Operation in Air to water “Cooling only” mode rated at 35°C ambient temperature, 50% R.H.; Entering water temperature 12°C, Outlet water temperature 7°C."]
["Notes","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C.","(2) - Operation in Air to water “Heating only” mode rated at 7°C ambient temperature, 85% R.H; Entering water temperature 40°C, Outlet water temperature 45°C."]
["Notes","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\".","(3) - Operation in Water to water “Cooling + Heating” mode rated with water flowing on cold and hot heat exchangers determined respectively at conditions for \"Cooling only\" and \"Heating only\"."]
["Notes","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C.","(4) - Chilled water outlet temperature 7°C, Hot water outlet temperature 45°C."]
["Notes","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating.","(5) - Sound power level are referred to condition (1) for Cooling and (2) for Heating."]
["Notes","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1","(6) - Sound power level (referred to evaporator 12/7°C, ambient 35°C full load operation) are measured in accordance with ISO 9614 and Eurovent 8/1"]
["Notes","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level.","(7) - The certification refers only to the overall sound power level."]
["Notes","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding","(8) - The sound pressure level is calculated from the sound power level and is for information only and not considered binding"]
["Notes","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options.","(9) - All data refers to the standard unit without options."]
["Notes","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data.","(10) - All data are subject to change without notice. Please refer to the unit nameplate data."]