{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYQ-BVP"]
[]
[]
[]
[]
["","","","","","EWYQ004BAVP","EWYQ005BAVP","EWYQ006BAVP","EWYQ008BAVP"]
["Cooling capacity","Nom.","","","kW","4.00 (1), 4.01 (2)"]
["Capacity control","Method","","","","Variable (inverter)"]
["Power input","Cooling","","Nom.","kW","1.27 (1), 0.840 (2)"]
["EER","","","","","3.14 (1), 4.80 (2)","3.06 (1), 4.51 (2)","3.15 (1), 5.35 (2)","3.1, 4.99 (2)"]
["Dimensions","Unit","","Depth","mm","350"]
["","","","Height","mm","735"]
["","","","Width","mm","1,090"]
["Weight","Unit","","","kg","83"]
["Casing","Colour","","","","Ivory white"]
["","Material","","","","Polyester painted galvanised steel plate"]
["Air heat exchanger","Type","","","","Cross fin coil/Hi-X tubes and chromate coated waffle louvre fins"]
["Fan","Quantity","","","","1"]
["","Type","","","","Propeller fan"]
["Compressor","Quantity","","","","1"]
["","Type","","","","Hermetically sealed swing compressor"]
["","Starting method","","","","Inverter driven"]
["Operation range","Air side","Cooling","Min.","°CDB","10"]
["","","","Max.","°CDB","43"]
["","Water side","Evaporator","Min.","°CDB","5"]
["","","","Max.","°CDB","22"]
["Sound power level","Cooling","","Nom.","dBA","63 (1)"]
["Sound pressure level","Cooling","","Nom.","dBA","48 (9)"]
["Refrigerant","Type","","","","R-410A"]
["","GWP","","","","2,088"]
["","Circuits","","Quantity","","1"]
["Power supply","Phase","","","","1N~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","230"]
["","Voltage range","","Min.","%","0"]
["","","","Max.","%","10"]
["Unit","Starting current","","Max","A","15.7 (11)"]
["","Running current","","Max","A","15.7"]
["Notes","","","","","(1) - Cooling: entering evaporator water temp. 12°C; leaving evaporator water temp. 7°C; ambient air temp. 35°C","(1) - Cooling: entering evaporator water temp. 12°C; leaving evaporator water temp. 7°C; ambient air temp. 35°C","(1) - Cooling: entering evaporator water temp. 12°C; leaving evaporator water temp. 7°C; ambient air temp. 35°C","(1) - Cooling: entering evaporator water temp. 12°C; leaving evaporator water temp. 7°C; ambient air temp. 35°C"]
["","","","","","(2) - Cooling: entering evaporator water temp. 23°C; leaving evaporator water temp. 18°C; ambient air temp. 35°C; standard: non-Eurovent","(2) - Cooling: entering evaporator water temp. 23°C; leaving evaporator water temp. 18°C; ambient air temp. 35°C; standard: non-Eurovent","(2) - Cooling: entering evaporator water temp. 23°C; leaving evaporator water temp. 18°C; ambient air temp. 35°C; standard: non-Eurovent","(2) - Cooling: entering evaporator water temp. 23°C; leaving evaporator water temp. 18°C; ambient air temp. 35°C; standard: non-Eurovent"]
["","","","","","(3) - Heating: entering condenser water temp. 40°C; leaving condenser water temp. 45°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent","(3) - Heating: entering condenser water temp. 40°C; leaving condenser water temp. 45°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent","(3) - Heating: entering condenser water temp. 40°C; leaving condenser water temp. 45°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent","(3) - Heating: entering condenser water temp. 40°C; leaving condenser water temp. 45°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent"]
["","","","","","(4) - Heating: entering condenser water temp. 30°C; leaving condenser water temp. 35°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent","(4) - Heating: entering condenser water temp. 30°C; leaving condenser water temp. 35°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent","(4) - Heating: entering condenser water temp. 30°C; leaving condenser water temp. 35°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent","(4) - Heating: entering condenser water temp. 30°C; leaving condenser water temp. 35°C; ambient air temp. 7°CDB, 6°CWB; standard: Eurovent"]
["","","","","","(5) - All performance calculations are strictly according to Eurovent standard","(5) - All performance calculations are strictly according to Eurovent standard","(5) - All performance calculations are strictly according to Eurovent standard","(5) - All performance calculations are strictly according to Eurovent standard"]
["","","","","","(6) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(6) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(6) - For average climate and low temperature application","(6) - For average climate and low temperature application"]
["","","","","","(7) - Including piping + PHE; excluding expansion vessel","(7) - Including piping + PHE; excluding expansion vessel","(7) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(7) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(8) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(8) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(8) - Including piping + PHE; excluding expansion vessel","(8) - Including piping + PHE; excluding expansion vessel"]
["","","","","","(9) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(9) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(9) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(9) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C"]
["","","","","","(10) - Assembly ≤ category I: excluded from 2014/68/EU due to article 1, 2f","(10) - Assembly ≤ category I: excluded from 2014/68/EU due to article 1, 2f","(10) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(10) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(11) - Inverter controlled compressor starting current always <= max. running current","(11) - Inverter controlled compressor starting current always <= max. running current","(11) - Assembly ≤ category I: excluded from 2014/68/EU due to article 1, 2f","(11) - Assembly ≤ category I: excluded from 2014/68/EU due to article 1, 2f"]
["Cooling capacity","Nom.","","","kW","","4.93 (1), 5.07 (2)","5.88 (1), 6.07 (2)","7.95 (1), 8.23 (2)"]
["Capacity control","Method","","","","","Variable (inverter)","Variable (inverter)","Variable (inverter)"]
["Power input","Cooling","","Nom.","kW","","1.61 (1), 1.12 (2)","1.87 (1), 1.13 (2)","2.57 (1), 1.65 (2)"]
["Dimensions","Unit","","Depth","mm","","350","380","380"]
["","","","Height","mm","","735","997","997"]
["","","","Width","mm","","1090","1160","1160"]
["Weight","Unit","","","kg","","83","106","106"]
["Casing","Colour","","","","","Ivory white","Ivory white","Ivory white"]
["","Material","","","","","Polyester painted galvanised steel plate","Painted galvanized steel plate","Painted galvanized steel plate"]
["Air heat exchanger","Type","","","","","Cross fin coil/Hi-X tubes and chromate coated waffle louvre fins","Cross fin coil/Hi-X tubes and PE coated waffle louvre fins","Cross fin coil/Hi-X tubes and PE coated waffle louvre fins"]
["Fan","Quantity","","","","","1","1","1"]
["","Type","","","","","Propeller fan","Propeller fan","Propeller fan"]
["Compressor","Quantity","","","","","1","1","1"]
["","Type","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["","Starting method","","","","","Inverter driven","Inverter driven","Inverter driven"]
["Operation range","Air side","Cooling","Min.","°CDB","","10","10","10"]
["","","","Max.","°CDB","","43","46","46"]
["","Water side","Evaporator","Min.","°CDB","","5","5","5"]
["","","","Max.","°CDB","","22","22","22"]
["Sound power level","Cooling","","Nom.","dBA","","64 (1)","69 (1)","69 (1)"]
["Sound pressure level","Cooling","","Nom.","dBA","","49 (9)","52 (10)","53 (10)"]
["Refrigerant","Type","","","","","R-410A","R-410A","R-410A"]
["","GWP","","","","","2088","2087.5","2087.5"]
["","Circuits","","Quantity","","","1","1","1"]
["Energy Efficiency Range","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Power supply","Phase","","","","","1N~","1N~","1N~"]
["","Frequency","","","Hz","","50","50","50"]
["","Voltage","","","V","","230","230","230"]
["","Voltage range","","Min.","%","","0","-10","-10"]
["","","","Max.","%","","10","10","10"]
["Unit","Starting current","","Max","A","","15.7 (11)","19.9 (12)","19.9 (12)"]
["","Running current","","Max","A","","15.7","19.9","19.9"]
["Fan motor","Drive","","","","","","Direct drive","Direct drive"]
["Notes","","","","","","","(12) - Inverter controlled compressor starting current always <= max. running current","(12) - Inverter controlled compressor starting current always <= max. running current"]
["","","","","","","","(13) - Ssc: Short-circuit power","(13) - Ssc: Short-circuit power"]
["","","","","","","","(14) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase.","(14) - European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current larger than 16A and ≤ 75A per phase."]