{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG140L7Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Space cooling","SEER","","","","","","","","","","5.10","5.10","6.72","","","","","","6.44","9.70"]
["","Annual energy consumption","","kWh/a","","","","","","","","467","467","355","","","","","","1,249","829"]
["","Capacity","Pdesign","kW","","","","","","","","6.80","6.80","6.80","","","","","","13.4","13.4"]
["","Energy efficiency class","","","","","","","","","","A","A","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","","","","6.00","6.00","6.33","","","","","","11.6","12.0"]
["","SCOP/A","","","","","","","","","","3.80","3.80","4.20","","","","","","4.27","3.96"]
["","Energy efficiency class","","","","","","","","","","A","A","A+"]
["","Annual energy consumption","","kWh/a","","","","","","","","2,211","2,211","2,110","","","","","","3,795","4,235"]
["Notes","","","","","","","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","","","","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","","","","","","","","(3) - EER/COP according to Eurovent 2012, for use outside EU only","","(3) - EER/COP according to Eurovent 2012, for use outside EU only","","","","","","(3) - EER/COP according to Eurovent 2012, for use outside EU only","(3) - EER/COP according to Eurovent 2012, for use outside EU only"]
["Cooling capacity","Nom.","","kW","","","","","","","","","","6.80 (1)","","","","","","13.4 (1)","13.4 (1)"]
["Nominal efficiency","EER","","","","","","","","","","","","3.39 (3)","","","","","","2.50 (3)","4.29 (3)"]
["","Annual energy consumption","","kWh","","","","","","","","","","1,005"]
["","COP","","","","","","","","","","","","3.97 (3)","","","","","","3.61 (3)"]
["","Energy labeling Directive","Cooling","","","","","","","","","","","A"]
["","","Heating","","","","","","","","","","","A"]
["Heating capacity","Nom.","","kW","","","","","","","","","","7.50 (2)","","","","","","15.5 (2)","15.5 (2)"]
["Outdoor unit","","","","","","","","","","","","","","RZQG71L8Y1","RZQG100L8Y1","RZQG100L8Y1","RZQG125L8Y1","RZQG125L8Y1"]
["Space cooling","Energy efficiency class","","","","","","","","","","","","","A++","A","A++","A","A+"]
["","Capacity","Pdesign","kW","","","","","","","","","","","6.80","9.50","9.50","12.0","12.00"]
["","SEER","","","","","","","","","","","","","6.72","5.10","6.80","5.10","6.00"]
["","Annual energy consumption","","kWh/a","","","","","","","","","","","355","652","489","824","700"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","","","","","","A+","A","A++","A","A+"]
["","Capacity","Pdesign","kW","","","","","","","","","","","6.33","11.3","11.30","12.7","12.66"]
["","SCOP/A","","","","","","","","","","","","","4.20","3.80","4.61","3.80","4.10"]
["","Annual energy consumption","","kWh/a","","","","","","","","","","","2110","4164","3432","4683","4323"]
["Space cooling","ηs,c","","%","","","","","","","","","","","","","","","","254.6","385.1"]
["Space heating (Average climate)","ηs,h","","%","","","","","","","","","","","","","","","","167.6","155.2"]