{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F / RZAG-LV1"]
[]
[]
[]
[]
["","","","","FCAHG71FVEB / RZAG71L7V1B","FCAHG125FVEB / RZAG125L7V1B","FCAHG140FVEB / RZAG140L7V1B","FCAHG100FVEB / RZAG100L7V1B (Archived)"]
["Cooling capacity","Nom.","","kW","6.8","12.0","13.4","9.5"]
["Space cooling","SEER","","","7.35 (2)","6.94 (2)","","7.35 (2)"]
["","Annual energy consumption","","kWh/a","324","605","","452"]
["","Capacity","Pdesign","kW","6.80","12.00","","9.50"]
["","Energy efficiency class","","","A++","A++","","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","5.65","9.52","","9.13"]
["","SCOP/A","","","4.54 (2)","4.63 (2)","","4.64 (2)"]
["","Energy efficiency class","","","A+","A++","","A++"]
["","Annual energy consumption","","kWh/a","1,743","2,879","","2,753"]
["Nominal efficiency","EER","","","4.09","4.00","3.35","4.42"]
["","Annual energy consumption","","kWh","830","1,500","2,000","1,075"]
["","COP","","","4.80","4.40","4.12","4.99"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","7.5","13.5","15.5","10.8"]
["Notes","","","","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","(2) - SEER and SCOP are according to EN 14825","(2) - SEER and SCOP are according to EN 14825","","(2) - SEER and SCOP are according to EN 14825"]
["","","","","","","(1) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]