{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":13,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / 2MXM-M9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / FDXM25F3V1B / 2MXM50M2V1B9","FDXM25F3V1B / FDXM35F3V1B / 2MXM50M2V1B9","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM50M3V1B9","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM50M3V1B9","FDXM25F3V1B9 / FDXM50F3V1B9 / 2MXM50M3V1B9","FDXM35F3V1B / FDXM35F3V1B / 2MXM50M2V1B9","FDXM35F3V1B / FDXM50F3V1B / 2MXM50M2V1B9","FDXM35F3V1B9 / FDXM35F3V1B9 / 2MXM50M3V1B9","FDXM35F3V1B9 / FDXM50F3V1B9 / 2MXM50M3V1B9"]
["Cooling capacity","Nom.","","kW","5.0","5.0","5.00","5.00","5.00","5.0","5.0","5.00","5.00"]
["Space cooling","SEER","","","6.21","6.24","6.21","6.24","6.51","6.41","6.40","6.41","6.40"]
["","Annual energy consumption","","kWh/a","282","281","282","281","269","273","274","273","274"]
["","Capacity","Pdesign","kW","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20"]
["","SCOP/A","","","3.78","3.79","3.78","3.79","3.86","3.82","3.89","3.82","3.89"]
["","Energy efficiency class","","","A","A","A","A","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","1,555","1,550","1,555","1,550","1,523","1,538","1,509","1,538","1,509"]
["Nominal efficiency","Annual energy consumption","","kWh","780","770","779","769","712","761","704","760","704"]
["","EER","","","3.21","3.25","3.21","3.25","3.51","3.29","3.55","3.29","3.55"]
["","COP","","","3.66","3.64","3.66","3.64","3.61","3.62","3.61","3.62","3.61"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Min.","","kW","5.60","5.60","","","","5.60","5.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Space heating (Average climate)","Pdh Heating capacity at -10°","","kW","","","3.42","3.43","3.55","","","3.44","3.57"]
["Heating capacity","Nom.","","kW","","","5.60","5.60","5.60","","","5.60","5.60"]
["Notes","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]