{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-M9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / RXM25M3V1B9","FDXM35F3V1B / RXM35M3V1B9","FDXM50F3V1B / RXM50M3V1B9","FDXM60F3V1B / RXM60M3V1B9"]
["Cooling capacity","Min.","","kW","","1.40","","1.70"]
["","Max.","","kW","","3.80","","6.50"]
["","Nom.","","kW","","3.40","","6.00"]
["Space cooling","SEER","","","","5.26","","5.56"]
["","Annual energy consumption","","kWh/a","","226","","315"]
["","Capacity","Pdesign","kW","","3.40","","6.00"]
["","Energy efficiency class","","","","A","","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","2.90","","4.60"]
["","SCOP/A","","","","3.88","","3.80"]
["","Energy efficiency class","","","","A","","A"]
["","Annual energy consumption","","kWh/a","","1,046","","1,693"]
["Nominal efficiency","EER","","","","2.98","","2.93"]
["","Annual energy consumption","","kWh","","570","","1,024"]
["","COP","","","","3.48","","3.21"]
["","Energy labeling Directive","Cooling","","","C","","C"]
["","","Heating","","","B","","C"]
["Heating capacity","Nom.","","kW","","4.00","","7.00"]
["","Min.","","kW","","1.40","","1.70"]
["","Max.","","kW","","5.00","","7.10"]
["Notes","","","","","(1) - See separate drawing for electrical data","","(1) - See separate drawing for operation range"]
["","","","","","(2) - See separate drawing for operation range","","(2) - See separate drawing for electrical data"]
["","","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Outdoor unit","","","","RXM25M3V1B9","","RXM50M3V1B9"]
["Cooling capacity","Min.","","kW","1.30","","1.70"]
["","Nom.","","kW","2.40","","5.00"]
["","Max.","","kW","3.00","","5.30"]
["Heating capacity","Min.","","kW","1.30","","1.70"]
["","Nom.","","kW","3.20","","5.80"]
["","Max.","","kW","4.50","","6.00"]
["Nominal efficiency","EER","","","3.77","","3.06"]
["","COP","","","4.00","","3.10"]
["","Annual energy consumption","","kWh","318","","816"]
["","Energy labeling Directive","Cooling","","A","","B"]
["","","Heating","","A","","D"]
["Space cooling","Energy efficiency class","","","A+","","A+"]
["","Capacity","Pdesign","kW","2.40","","5.00"]
["","SEER","","","5.68","","5.77"]
["","Annual energy consumption","","kWh/a","148","","303"]
["Space heating (Average climate)","Energy efficiency class","","","A+","","A"]
["","Capacity","Pdesign","kW","2.60","","4.00"]
["","SCOP/A","","","4.24","","3.93"]
["","Pdh Heating capacity at -10°","","kW","2.16","","3.55"]
["","Annual energy consumption","","kWh/a","858","","1424"]