{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":11,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM40A2V1B9","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM40A2V1B9","FDXM25F3V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B9","FDXM35F3V1B9 / FDXM50F3V1B9 / 2MXM50A2V1B9","FDXM35F3V1B9 / FDXM35F3V1B9 / 2MXM68A2V1B9","FDXM25F3V1B9 / FDXM25F3V1B9 / 2MXM50A2V1B9 (Archived)","FDXM25F3V1B9 / FDXM35F3V1B9 / 2MXM50A2V1B9 (Archived)"]
["Cooling capacity","Nom.","","kW","4.00","4.00","5.00","5.00"]
["Heating capacity","Nom.","","kW","4.20","4.20","5.60","5.60"]
["Nominal efficiency","Annual energy consumption","","kWh","563","556","712","704"]
["","COP","","","4.13","4.17","3.61","3.61"]
["","EER","","","3.55","3.60","3.51","3.55"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","223","228","269","273"]
["","Energy efficiency class","","","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","4.00","4.00","5.00","5.00"]
["","SEER","","","6.28","6.16","6.52","6.40"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","1,117","1,106","1,529","1,514"]
["","Capacity","Pdesign","kW","3.20","3.20","4.20","4.20"]
["","Energy efficiency class","","","A+","A+","A","A"]
["","Pdh Heating capacity at -10°","","kW","2.61","2.62","3.27","3.31"]
["","SCOP/A","","","4.01","4.05","3.85","3.88"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","6.8","5.00","5.00"]
["Heating capacity","Nom.","","kW","","","","","8.60","5.60","5.60"]
["Nominal efficiency","EER","","","","","","","2.73","3.21","3.25"]
["","COP","","","","","","","3.01","3.66","3.64"]
["","Annual energy consumption","","kWh","","","","","1245","779","769"]
["Space cooling","Energy efficiency class","","","","","","","A","A++","A++"]
["","Capacity","Pdesign","kW","","","","","6.80","5.00","5.00"]
["","SEER","","","","","","","5.43","6.22","6.25"]
["","Annual energy consumption","","kWh/a","","","","","438","281","280"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","A","A","A"]
["","Capacity","Pdesign","kW","","","","","3.60","4.20","4.20"]
["","SCOP/A","","","","","","","3.81","3.80","3.80"]
["","Pdh Heating capacity at -10°","","kW","","","","","3.10","2.92","2.94"]
["","Annual energy consumption","","kWh/a","","","","","1323","1548","1548"]
["Energy Efficiency Range","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Nominal efficiency","Energy labeling Directive","Cooling","","","","","","","A","A"]
["","","Heating","","","","","","","A","A"]