{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A9"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / RXM35A5V1B9","FDXM50F3V1B9 / RXM50A5V1B9"]
["Cooling capacity","Min.","","kW","1.4","1.7"]
["","Nom.","","kW","3.4","5"]
["","Max.","","kW","3.8","5.3"]
["Heating capacity","Min.","","kW","1.4","1.7"]
["","Nom.","","kW","4","5.8"]
["","Max.","","kW","5","6"]
["Nominal efficiency","EER","","","2.98","3.06"]
["","COP","","","3.48","3.1"]
["","Annual energy consumption","","kWh","570","817"]
["","Energy labeling Directive","Cooling","","C","B"]
["","","Heating","","B","D"]
["Space cooling","Energy efficiency class","","","A","A+"]
["","Capacity","Pdesign","kW","3.4","5"]
["","SEER","","","5.35","5.77"]
["","Annual energy consumption","","kWh/a","222","303"]
["Space heating (Average climate)","Energy efficiency class","","","A","A"]
["","Capacity","Pdesign","kW","2.9","4"]
["","SCOP/A","","","3.95","3.93"]
["","Pdh Heating capacity at -10°","","kW","2.32","3.54"]
["","Annual energy consumption","","kWh/a","1028","1424"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - See separate drawing for operation range"]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - See separate drawing for electrical data"]