{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZAG-MY1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZAG71M7Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZAG100M7Y1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","9.50 (1)"]
["Space cooling","SEER","","","6.32","8.60"]
["","Annual energy consumption","","kWh/a","377","387"]
["","Capacity","Pdesign","kW","6.80","9.50"]
["","Energy efficiency class","","","A++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.70","7.80"]
["","SCOP/A","","","4.28","4.51"]
["","Energy efficiency class","","","A+","A+"]
["","Annual energy consumption","","kWh/a","1,537","2,421"]
["Heating capacity","Nom.","","kW","7.50 (2)","10.8 (2)"]
["Notes","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data"]