{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG125L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG125L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM60F3V1B9 / FDXM60F3V1B9 / RZQG125L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG71L8Y1B"]
["Cooling capacity","Nom.","","kW","","","","","","","","6.80","6.80","6.80"]
["Space cooling","SEER","","","","","","","","","","4.80","4.80","4.80"]
["","Annual energy consumption","","kWh/a","","","","","","","","496","496","496"]
["","Capacity","Pdesign","kW","","","","","","","","6.80","6.80","6.80"]
["","Energy efficiency class","","","","","","","","","","B","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Energy efficiency class","","","","","","","","","","A","A","A"]
["","Annual energy consumption","","kWh/a","","","","","","","","2,211","2,211","2,211"]
["Nominal efficiency","EER","","","","","","","","","","3.06","3.06","3.06"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range"]
["","","","","","","","","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data"]
["","","","","","","","","","","","","(3) - See separate drawing for operation range"]
["","","","","","","","","","","","","(4) - See separate drawing for electrical data"]