{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":9,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Sound pressure level","Heating","","High","dBA","35.0","35.0","","38.0"]
["","","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Low","dBA","27.0","27.0","","30.0"]
["","Cooling","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Low","dBA","27.0","27.0","","30.0"]
["","","","High","dBA","35.0","35.0","","38.0"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Insulation for fitting","","","","1","1","1","1"]
["","Sealing pad","","","","1","1","1","1"]
["","Clamp metal","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8"]
["","Sealing material","","","","2","2","2","2"]
["","Clamps","","","","6","6","6","6"]
["","Washer fixing plate","","","","4","4","4","4"]
["","Screws for duct flanges","","","","1","1","1","1"]
["","Air filter","","","","1","1","1","1"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gas","","OD","mm","9.50","9.50","","12.70"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Cooling","","Nom.","kW","0.036","0.036","","0.060"]
["","Heating","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Cooling","","","dBA","53.0","53.0","","56.0"]
["","Heating","","","dBA","53.0","53.0","","56.0"]
["Dimensions","Unit","","Width","mm","750","750","","1,150"]
["","","","Depth","mm","620","620","","620"]
["","","","Height","mm","200","200","","200"]
["Weight","Unit","","","kg","21","21","","28"]
["Fan","External static pressure","","Nom.","Pa","30","30","","40"]
["","Air flow rate","Heating","High","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Low","m³/min","7.3","7.3","","13.5"]
["","","Cooling","Low","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","High","m³/min","8.7","8.7","","16.0"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Frequency","","","Hz","50","50","","50"]
["","Voltage","","","V","220-240","220-240","","220-240"]
["Notes","","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data","","(1) - See separate drawing for electrical data"]
["Power input","Cooling","","Nom.","kW","","","0.060"]
["","Heating","","Nom.","kW","","","0.060"]
["Dimensions","Unit","","Height","mm","","","200"]
["","","","Width","mm","","","1150"]
["","","","Depth","mm","","","620"]
["Weight","Unit","","","kg","","","28"]
["Fan","Air flow rate","Cooling","High","m³/min","","","15.8"]
["","","","Medium","m³/min","","","14.6"]
["","","","Low","m³/min","","","13.3"]
["","","Heating","High","m³/min","","","15.8"]
["","","","Medium","m³/min","","","14.6"]
["","","","Low","m³/min","","","13.3"]
["","External static pressure","","Nom.","Pa","","","40"]
["Sound power level","Cooling","","","dBA","","","55.0"]
["","Heating","","","dBA","","","55.0"]
["Sound pressure level","Cooling","","High","dBA","","","38.0"]
["","","","Medium","dBA","","","35.0"]
["","","","Low","dBA","","","30.0"]
["","Heating","","High","dBA","","","38.0"]
["","","","Medium","dBA","","","35.0"]
["","","","Low","dBA","","","30.0"]
["Piping connections","Liquid","","OD","mm","","","6.35"]
["","Gas","","OD","mm","","","12.70"]
["","Drain","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Power supply","Phase","","","","","","1~"]
["","Frequency","","","Hz","","","50"]
["","Voltage","","","V","","","220-240"]