{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25L3V1B","FDXS35F2VEB / RXS35L3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4"]
["","Max.","","kW","3.0","3.8"]
["","Nom.","","kW","2.4 (2)","3.4 (2)"]
["Space cooling","SEER","","","5.63","5.21"]
["","Annual energy consumption","","kWh/a","149","228"]
["","Capacity","Pdesign","kW","2.40","3.40"]
["","Energy efficiency class","","","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.60","2.90"]
["","SCOP/A","","","4.24","3.88"]
["","Energy efficiency class","","","A+","A"]
["","Annual energy consumption","","kWh/a","858","1,047"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5"]
["","Drain","OD","mm","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["Nominal efficiency","Annual energy consumption","","kWh","321","574"]
["","EER","","","3.74 (1)","2.96 (1)"]
["","COP","","","4.00 (1)","3.48 (1)"]
["","Energy labeling Directive","Cooling","","A","B"]
["","","Heating","","A","A"]
["Heating capacity","Nom.","","kW","3.2 (2)","4.0 (2)"]
["","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.5","5.0"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]