{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V"]
[]
[]
[]
[]
["","","","","FFQ25B9V1B (Archived)","FFQ35B9V1B (Archived)","FFQ50B9V1B (Archived)","FFQ60B9V1B (Archived)"]
["Sound pressure level","Cooling","Low","dBA","24.5","25","27","32"]
["","","High","dBA","29.5","32","36","41"]
["Standard Accessories","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Paper pattern for installation","","","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation"]
["","Drain hose","","","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp metal","","","Clamp metal","Clamp metal","Clamp metal","Clamp metal"]
["","Washer fixing plate","","","Washer fixing plate","Washer fixing plate","Washer fixing plate","Washer fixing plate"]
["","Sealing pads","","","Sealing pads","Sealing pads","Sealing pads","Sealing pads"]
["","Clamps","","","Clamps","Clamps","Clamps","Clamps"]
["","Screws","","","Screws","Screws","Screws","Screws"]
["","Washer for hanger bracket","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Insulation for fitting","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["Cooling capacity","Total capacity","Nom.","kW","2.5 (1)","3.4 (1)","4.7 (1)","5.8 (1)"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Cooling","","dBA","46.5","49","53","58"]
["Dimensions","Unit","Width","mm","575","575","575","575"]
["","","Depth","mm","575","575","575","575"]
["","","Height","mm","286","286","286","286"]
["Casing","Material","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["","Colour","","","Unpainted","Unpainted","Unpainted","Unpainted"]
["Weight","Unit","","kg","17.5","17.5","17.5","17.5"]
["Decoration panel","Weight","","kg","2.7","2.7","2.7","2.7"]
["","Model","","","BYFQ60BW1","BYFQ60BW1","BYFQ60BW1","BYFQ60BW1"]
["","Dimensions","Height","mm","55","55","55","55"]
["","","Depth","mm","700","700","700","700"]
["","","Width","mm","700","700","700","700"]
["","Colour","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Heating capacity","Total capacity","Nom.","kW","3.2 (2)","4.5 (2)","5.5 (2)","7.0 (2)"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - Nominal cooling and heating capactity is depending on the outdoor unit type","(4) - Nominal cooling and heating capactity is depending on the outdoor unit type","(4) - Nominal cooling and heating capactity is depending on the outdoor unit type","(4) - Nominal cooling and heating capactity is depending on the outdoor unit type"]
["","","","","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(5) - PED unit category: Art3§3: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]