{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":23,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FHA100AVEB8 / RZASG100M7Y1B","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZASG100M7Y1B","FHA50AVEB9 / FHA50AVEB9 / RZASG100M7Y1B","FHA35AVEB99 / FHA35AVEB99 / FHA35AVEB99 / RZASG100M7Y1B","FHA50AVEB99 / FHA50AVEB99 / RZASG100M7Y1B","FHA35AVEB98 / FHA35AVEB98 / FHA35AVEB98 / RZASG100M7Y1B","FHA50AVEB98 / FHA50AVEB98 / RZASG100M7Y1B","FHA125AVEB / RZASG125M7Y1B","FHA125AVEB9 / RZASG125M7Y1B","FHA125AVEB8 / RZASG125M7Y1B","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZASG125M7Y1B","FHA50AVEB9 / FHA50AVEB9 / FHA50AVEB9 / RZASG125M7Y1B","FHA60AVEB9 / FHA60AVEB9 / RZASG125M7Y1B","FHA140AVEB / RZASG140M7Y1B","FHA140AVEB9 / RZASG140M7Y1B","FHA140AVEB8 / RZASG140M7Y1B","FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / FHA35AVEB9 / RZASG140M7Y1B","FHA50AVEB9 / FHA50AVEB9 / FHA50AVEB9 / RZASG140M7Y1B","FHA71AVEB9 / FHA71AVEB9 / RZASG140M7Y1B"]
["Cooling capacity","Nom.","","kW","","","","","","","","12.1 (1)","12.1 (1)","12.1 (1)","12.1 (1)","","","13.4 (1)","13.4 (1)","13.4 (1)","13.4 (1)"]
["Space cooling","SEER","","","","","","","","","","5.83","5.83","5.83","7.21","","","5.88","5.88","5.88","8.88"]
["","Annual energy consumption","","kWh/a","","","","","","","","1,246","1,246","1,246","1,007","","","1,368","1,368","1,368","905"]
["","Capacity","Pdesign","kW","","","","","","","","12.1","12.1","12.1","12.1","","","13.4","13.4","13.4","13.4"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","","","","","","6.00","6.00","6.00","6.00","","","7.80","7.80","7.80","7.80"]
["","SCOP/A","","","","","","","","","","3.83","3.83","3.83","4.75","","","3.81","3.81","3.81","5.13"]
["","Annual energy consumption","","kWh/a","","","","","","","","2,193","2,193","2,193","1,768","","","2,866","2,866","2,866","2,129"]
["Heating capacity","Nom.","","kW","","","","","","","","13.5 (2)","13.5 (2)","13.5 (2)","13.5 (2)","","","15.5 (2)","15.5 (2)","15.5 (2)","15.5 (2)"]
["Cooling capacity","Nom.","","kW","9.5","9.50","9.50","9.50","9.50","9.50","9.50","","","","","12.1","12.1","","","","","13.4","13.4"]
["Heating capacity","Nom.","","kW","10.8","10.8","10.8","10.8","10.8","10.8","10.8","","","","","13.5","13.5","","","","","15.5","15.5"]
["Space cooling","Energy efficiency class","","","A+","A++","A+","A++","A+","A++","A+"]
["","Capacity","Pdesign","kW","9.5","9.50","9.50","9.50","9.50","9.50","9.50","","","","","12.1","12.1","","","","","13.4","13.4"]
["","SEER","","","5.83","7.26","5.79","7.26","5.79","7.26","5.79","","","","","6.52","6.73","","","","","8.19","8.68"]
["","Annual energy consumption","","kWh/a","570","458","574","458","574","458","574","","","","","1114","1079","","","","","981","926"]
["Space heating (Average climate)","Energy efficiency class","","","A","A+","A","A+","A","A+","A"]
["","Capacity","Pdesign","kW","6","6.00","6.00","6.00","6.00","6.00","6.00","","","","","6.00","6.00","","","","","7.80","7.80"]
["","SCOP/A","","","3.91","4.02","3.92","4.02","3.92","4.02","3.92","","","","","4.71","4.23","","","","","4.89","4.74"]
["","Annual energy consumption","","kWh/a","2148","2090","2143","2090","2143","2090","2143","","","","","1783","1984","","","","","2233","2302"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","","","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]