{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-B / RXB-B"]
[]
[]
[]
[]
["","","","","FTXB25B1V1 / RXB25B6V19","FTXB25B1V1 / RXB25B6V1","FTXB25BV1 / RXB25B5V1","FTXB35B1V1 / RXB35B6V19","FTXB35B1V1 / RXB35B6V1","FTXB35BV1 / RXB35B5V1","FTXB50BV1B / RXB50BV1B","FTXB60BV1B / RXB60BV1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.630","1.750"]
["","Max.","","kW","3.0","3.0","3.0","3.8","3.8","3.8","6.200","6.500"]
["","Nom.","","kW","2.5","2.5","2.5","3.5","3.5","3.5","5.480","6.230"]
["Space cooling","SEER","","","5.66","5.66","5.66","5.86","5.86","5.86","5.93","6.09"]
["","Annual energy consumption","","kWh/a","155","155","155","210","210","210","324","359"]
["","Capacity","Pdesign","kW","2.50","2.50","2.50","3.50","3.50","3.50","5.48","6.23"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.40","2.40","2.80","2.80","2.80","3.64","3.80"]
["","SCOP/A","","","4.24","4.24","4.24","4.16","4.16","4.16","4.27","4.06"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","793","793","793","943","943","943","1,195","1,311"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5","9.5","9.5","12.7","15.9"]
["","Drain","OD","mm","18.0","18.0","18.0","18.0","18.0","18.0","16.5","16.5"]
["Nominal efficiency","EER","","","3.42 (1)","3.42 (1)","3.42 (1)","3.37","3.37","3.37 (1)","3.19","3.23"]
["","Annual energy consumption","","kWh","365","365","365","519","519","519","859","966"]
["","COP","","","4.10 (1)","4.10 (1)","4.06 (1)","3.76 (1)","3.76 (1)","3.76 (1)","3.75","3.81"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","B","A"]
["","","Heating","","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.3","3.3","3.3","3.6","3.6","3.6","5.620","6.400"]
["","Min.","","kW","1.3","1.3","1.3","1.3","1.3","1.3","1.170","1.200"]
["","Max.","","kW","4.0","4.0","4.0","4.8","4.8","4.8","6.600","7.100"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(2) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","","","","","","","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","","","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]