{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":10,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-B"]
[]
[]
[]
[]
["","","","","FTXB25B1V1","FTXB25BV1","FTXB35B1V1","FTXB35BV1","FTXB50BV1B","FTXB60BV1B"]
["Sound pressure level","Heating","High","dBA","38","38","40","40","40","43"]
["","","Medium","dBA","33","","34"]
["","","Silent operation","dBA","25","25","23","23","32","33"]
["","","Low","dBA","28","28","26","26","35","37"]
["","Cooling","Medium","dBA","33","","34"]
["","","Silent operation","dBA","22","22","25","25","32","33"]
["","","Super high","dBA","","","","","44","46"]
["","","Low","dBA","25","25","26","26","35","37"]
["","","High","dBA","38","38","39","39","40","43"]
["","","Nom.","dBA","33","33","34","34","38","41"]
["","Cooling","Nom.","dBA","33","33","34","34","38","41"]
["Standard Accessories","Installation manual","","","1","1","1","1"]
["","Operation manual","","","1","1","1","1"]
["","Wireless remote control","","","1","","1"]
["","AA dry-cell batteries","","","2","","2"]
["","Remote control holder","","","1","1","1","1"]
["","Mounting plate","","","1","1","1","1"]
["","Indoor unit fixing screws","","","2","2","2","2"]
["Control systems","Infrared remote control","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","APGS02","APGS02"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","9.5","9.5"]
["","Drain","","","18","18","18","18"]
["Power input","Cooling","Nom.","kW","0.030","0.040","0.030","0.040"]
["","Heating","Nom.","kW","0.040","0.040","0.040","0.040"]
["Sound power level","Cooling","","dBA","52","52","53","53","55","61"]
["","Heating","","dBA","52","52","54","54"]
["Dimensions","Unit","Width","mm","770","770","770","770","1,065","1,065"]
["","","Depth","mm","216","216","216","216","224","224"]
["","","Height","mm","283","283","283","283","310","310"]
["Casing","Colour","","","","","","","White","White"]
["Weight","Unit","","kg","7","8","7","8","14","14"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Contains fluorinated greenhouse gases","(1) - SL: The silent fan level of the air flow rate setting","(1) - Contains fluorinated greenhouse gases","(1) - SL: The silent fan level of the air flow rate setting"]
["Standard Accessories","Infrared remote control","","","","1","","1"]
["","Batteries","","","","2","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","2","","2"]
["Notes","","","","","","","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice."]