{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-A"]
[]
[]
[]
[]
["","","","","FTXC25AV1B","FTXC35AV1B","FTXC50AV1B","FTXC60AV1B"]
["Sound pressure level","Cooling","Silent operation","dBA","21","22","32","33"]
["","","Super high","dBA","41","42","44","46"]
["","","Low","dBA","29","30","35","37"]
["","","High","dBA","40","41","40","43"]
["Standard Accessories","Installation manual","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Operation manual","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Wireless remote control","","","Wireless remote control","Wireless remote control","Wireless remote control","Wireless remote control"]
["","Batteries","","","Batteries","Batteries","Batteries","Batteries"]
["","Remote control holder","","","Remote control holder","Remote control holder","Remote control holder","Remote control holder"]
["","Mounting plate","","","Mounting plate","Mounting plate","Mounting plate","Mounting plate"]
["","Titanium apatite filters","","","Titanium apatite filters","Titanium apatite filters","Titanium apatite filters","Titanium apatite filters"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7","12.7"]
["","Drain","","","OD16,5","OD16,5","OD16,5","OD16,5"]
["Power input","Cooling","Nom.","kW","693","1,060","1,668","1,931"]
["","Heating","Nom.","kW","700","950","1,550","1,680"]
["Sound power level","Cooling","","dBA","53","54","55","61"]
["Dimensions","Unit","Width","mm","859","859","1,124","1,124"]
["","","Depth","mm","209","209","237","237"]
["","","Height","mm","288","288","310","310"]
["Casing","Material","","","High impact polystyrene","High impact polystyrene","High impact polystyrene","High impact polystyrene"]
["","Colour","","","White","White","White","White"]
["Weight","Unit","","kg","9.0","9.0","14.0","14.0"]
["Fan","External static pressure","High","Pa","0","0","0","0"]
["","","Nom.","Pa","0","0","0","0"]
["","","Low","Pa","0","0","0","0"]
["","","Super high","Pa","0","0","0","0"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]