{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXD-A / RXD-A"]
[]
[]
[]
[]
["","","","","FTXD25A5V1B / RXD25A5V1B","FTXD35A5V1B / RXD35A5V1B"]
["Outdoor unit","","","","RXD25A5V1B","RXD35A5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.5","3.3"]
["","Max.","","kW","3.2","3.9"]
["Heating capacity","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.8","3.5"]
["","Max.","","kW","4.4","5"]
["Nominal efficiency","EER","","","4.46","4.23"]
["","COP","","","4.59","3.98"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++"]
["","Capacity","Pdesign","kW","2.5","3.3"]
["","SEER","","","8.5","8.5"]
["","Annual energy consumption","","kWh/a","103","136"]
["Space heating (Average climate)","Energy efficiency class","","","A+++","A+++"]
["","Capacity","Pdesign","kW","2.4","2.5"]
["","SCOP/A","","","5.1","5.1"]
["","Pdh Heating capacity at -10°","","kW","2.12","2.19"]
["","Annual energy consumption","","kWh/a","659","686"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified"]
["","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]