{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-E / RXF-C"]
[]
[]
[]
[]
["","","","","FTXF20E5V1B / RXF20C5V1B","FTXF25E5V1B / RXF25C5V1B","FTXF35E5V1B / RXF35C5V1B","FTXF42E5V1B / RXF42C5V1B"]
["Outdoor unit","","","","RXF20C5V1B","RXF25C5V1B","RXF35C5V1B","RXF42C5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3","1.4"]
["","Nom.","","kW","2","2.5","3.3","4.2"]
["","Max.","","kW","2.4","2.8","3.8","4.3"]
["Heating capacity","Min.","","kW","1.3","1.3","1.3","1.4"]
["","Nom.","","kW","2.4","2.8","3.5","4.6"]
["","Max.","","kW","3.3","3.7","4.4","5"]
["Nominal efficiency","EER","","","3.38","3.24","3.3","3.3"]
["","COP","","","3.75","3.73","3.72","3.71"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","2","2.5","3.5","4.2"]
["","SEER","","","6.22","6.22","6.22","6.5"]
["","Annual energy consumption","","kWh/a","113","141","197","226"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","2.2","2.4","2.6","3.3"]
["","SCOP/A","","","4.11","4.11","4.11","4.3"]
["","Pdh Heating capacity at -10°","","kW","1.91","2","2.22","2.61"]
["","Annual energy consumption","","kWh/a","749","817","885","1075"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]