{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F / RXF-B"]
[]
[]
[]
[]
["","","","","FTXF60F2V1B / RXF60B2V1B","FTXF60F2V1B / RXF60B5V1B"]
["Outdoor unit","","","","RXF60B2V1B","RXF60B5V1B"]
["Cooling capacity","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","6","6"]
["","Max.","","kW","7","7"]
["Heating capacity","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","6.4","6.4"]
["","Max.","","kW","8","8"]
["Nominal efficiency","EER","","","3.25","3.25"]
["","COP","","","3.93","3.93"]
["","Annual energy consumption","","kWh","923","923"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++"]
["","Capacity","Pdesign","kW","6","6"]
["","SEER","","","6.15","6.15"]
["","Annual energy consumption","","kWh/a","342","342"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","4.8","4.8"]
["","SCOP/A","","","4.06","4.06"]
["","Pdh Heating capacity at -10°","","kW","4.24","4.24"]
["","Annual energy consumption","","kWh/a","1653","1653"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]