{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-JB / RXG-K"]
[]
[]
[]
[]
["","","","","FTXG25JV1BB / RXG25K3V1B","FTXG35JV1BB / RXG35K3V1B","FTXG50JV1BB / RXG50K3V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.5 (2)","3.5 (2)","5.0 (2)"]
["Space cooling","SEER","","","6.53","6.51","5.45"]
["","Annual energy consumption","","kWh/a","134","188","321"]
["","Capacity","Pdesign","kW","2.50","3.50","5.00"]
["","Energy efficiency class","","","A++","A++","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.80","3.30","4.60"]
["","SCOP/A","","","4.34","4.23","3.87"]
["","Energy efficiency class","","","A+","A+","A"]
["","Annual energy consumption","","kWh/a","903","1,091","1,660"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.7"]
["","Drain","OD","mm","16 or 18","16 or 18","18.0"]
["Nominal efficiency","EER","","","4.46 (1)","3.93 (1)","3.21 (1)"]
["","Annual energy consumption","","kWh","280","445","780"]
["","COP","","","4.36 (1)","4.04 (1)","3.63 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","3.4 (3)","4.0 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Max.","","kW","4.5","5.0","6.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(2) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(4) - 220V","(4) - 220V","(4) - 220V"]
["","","","","(5) - 230V","(5) - 230V","(5) - 230V"]
["","","","","(6) - 240V","(6) - 240V","(6) - 240V"]
["","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]