{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":9,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXK-AS"]
[]
[]
[]
[]
["","","","","","FTXK25AV1BS","FTXK35AV1BS","FTXK50AV1BS","FTXK60AV1BS"]
["Fan","Air flow rate","Cooling","Nom.","m³/min","7.68","7.98","13.32","16.56"]
["Sound pressure level","Cooling","","Nom.","dBA","34","34","38","41"]
["Fan","Air flow rate","Heating","Nom.","m³/min","7.68","7.98","13.32","16.56"]
["Sound pressure level","Heating","","Nom.","dBA","34","34","38","41"]
["Casing","Colour","","","","Silver","Silver","Silver","Silver"]
["Dimensions","Unit","","Height","mm","297","297","320","320"]
["","","","Width","mm","890","890","1172","1172"]
["","","","Depth","mm","210","210","242","242"]
["Weight","Unit","","","kg","9.0","9.0","14.0","14.0"]
["Fan","Air flow rate","Cooling","High","m³/min","9.78","10.14","15.00","18.54"]
["","","","Low","m³/min","6.06","6.54","11.82","14.34"]
["","","","Silent operation","m³/min","4.68","4.68","10.62","12.36"]
["","","Heating","High","m³/min","9.78","10.14","15.00","18.54"]
["","","","Low","m³/min","6.06","6.54","11.82","14.34"]
["","","","Silent operation","m³/min","4.68","4.68","10.62","12.36"]
["Sound power level","Cooling","","","dBA","53","54","55","61"]
["","Heating","","","dBA","53","54","55","61"]
["Sound pressure level","Cooling","","Super high","dBA","41","42","44","46"]
["","","","High","dBA","40","41","40","43"]
["","","","Low","dBA","29","30","35","37"]
["","","","Silent operation","dBA","21","22","32","33"]
["","Heating","","High","dBA","40","41","40","43"]
["","","","Low","dBA","29","30","35","37"]
["","","","Silent operation","dBA","21","22","32","33"]
["Refrigerant","GWP","","","","2087.5","2087.5","2087.5","2087.5"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.52","9.52","12.70","15.90"]
["Power supply","Name","","","","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240"]