{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXK-AW / RXK-A"]
[]
[]
[]
[]
["","","","","FTXK25AV1BW / RXK25AV1B","FTXK35AV1BW / RXK35AV1B","FTXK50AV1BW / RXK50AV1B","FTXK60AV1BW / RXK60AV1B"]
["Cooling capacity","Min.","","kW","1.300","1.300","1.630","1.750"]
["","Max.","","kW","3.000","3.800","6.200","6.500"]
["","Nom.","","kW","2.500 (2)","3.500 (2)","5.480 (2)","6.230 (2)"]
["Space cooling","SEER","","","5.66","5.86","5.93","6.09"]
["","Annual energy consumption","","kWh/a","155","209","324","359"]
["","Capacity","Pdesign","kW","2.50","3.50","5.48","6.23"]
["","Energy efficiency class","","","A+","A+","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.40","2.80","3.37","3.80"]
["","SCOP/A","","","4.24","4.16","4.01","4.06"]
["","Energy efficiency class","","","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","792","945","1,177","1,310"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.70","15.90"]
["Nominal efficiency","EER","","","3.42 (1)","3.26 (1)","3.22 (1)","3.23 (1)"]
["","Annual energy consumption","","kWh","365","537","851","964"]
["","COP","","","3.67 (1)","3.76 (1)","3.63 (1)","3.81 (1)"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","3.300 (2)","3.600 (2)","5.620 (2)","6.400 (2)"]
["","Min.","","kW","1.300","1.300","1.170","1.200"]
["","Max.","","kW","4.000","4.750","6.600","8.000"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(3) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(3) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(3) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","(4) - All specifications are subjected to change by the manufacturer without prior notice.","(4) - All specifications are subjected to change by the manufacturer without prior notice.","(4) - All specifications are subjected to change by the manufacturer without prior notice.","(4) - All specifications are subjected to change by the manufacturer without prior notice."]