{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 4MWXM-A"]
[]
[]
[]
[]
["","","","","FTXM25R2V1B / FTXM25R2V1B / 4MWXM52A2V1B (Archived)","FTXM25R5V1B / FTXM25R5V1B / 4MWXM52A2V1B (Archived)"]
["Cooling capacity","Nom.","","kW","5.00","5.00"]
["Heating capacity","Nom.","","kW","6.80","6.80"]
["Nominal efficiency","EER","","","4.85","4.85"]
["","COP","","","4.45","4.45"]
["","Annual energy consumption","","kWh","515","515"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++"]
["","Capacity","Pdesign","kW","5.00","5.00"]
["","SEER","","","8.59","8.59"]
["","Annual energy consumption","","kWh/a","204","204"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+"]
["","Capacity","Pdesign","kW","4.80","4.80"]
["","SCOP/A","","","4.38","4.38"]
["","Pdh Heating capacity at -10°","","kW","3.82","3.82"]
["","Annual energy consumption","","kWh/a","1533","1533"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]