{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":9,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-R9"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / RXM20R5V1B9","FTXM20R2V1B / RXM20R5V1B9","FTXM25R5V1B / RXM25R5V1B9","FTXM25R2V1B / RXM25R5V1B9","FTXM35R5V1B / RXM35R5V1B9"]
["Cooling capacity","Min.","","kW","1.30","","1.30","","1.40"]
["","Nom.","","kW","2.00","","2.50","","3.40"]
["","Max.","","kW","2.60","","3.20","","4.00"]
["Heating capacity","Min.","","kW","1.30","","1.30","","1.40"]
["","Nom.","","kW","2.50","","2.80","","4.00"]
["","Max.","","kW","3.50","","4.70","","5.20"]
["Nominal efficiency","Annual energy consumption","","kWh","219","","278","","402"]
["","COP","","","5.00","","5.00","","4.04"]
["","EER","","","4.57","","4.50","","4.23"]
["","Energy labeling Directive","Cooling","","A","","A","","A"]
["","","Heating","","A","","A","","A"]
["Space cooling","Annual energy consumption","","kWh/a","81","","101","","137"]
["","Energy efficiency class","","","A+++","","A+++","","A+++"]
["","Capacity","Pdesign","kW","2.00","","2.50","","3.40"]
["","SEER","","","8.65","","8.65","","8.65"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","631","","659","","686"]
["","Capacity","Pdesign","kW","2.30","","2.40","","2.50"]
["","Energy efficiency class","","","A+++","","A+++","","A+++"]
["","Pdh Heating capacity at -10°","","kW","2.24","","2.30","","2.35"]
["","SCOP/A","","","5.10","","5.10","","5.10"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Min.","","kW","","1.3","","1.3"]
["","Nom.","","kW","","2","","2.5"]
["","Max.","","kW","","2.6","","3.2"]
["Heating capacity","Min.","","kW","","1.3","","1.3"]
["","Nom.","","kW","","2.5","","2.8"]
["","Max.","","kW","","3.5","","4.7"]
["Nominal efficiency","EER","","","","4.57","","4.5"]
["","COP","","","","5","","5"]
["","Annual energy consumption","","kWh","","219","","278"]
["","Energy labeling Directive","Cooling","","","A","","A"]
["","","Heating","","","A","","A"]
["Space cooling","Energy efficiency class","","","","A+++","","A+++"]
["","Capacity","Pdesign","kW","","2","","2.5"]
["","SEER","","","","8.65","","8.65"]
["","Annual energy consumption","","kWh/a","","81","","101"]
["Space heating (Average climate)","Energy efficiency class","","","","A+++","","A+++"]
["","Capacity","Pdesign","kW","","2.3","","2.4"]
["","SCOP/A","","","","5.1","","5.1"]
["","Pdh Heating capacity at -10°","","kW","","2.24","","2.3"]
["","Annual energy consumption","","kWh/a","","631","","659"]