{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-MB9 / RXN-MB9"]
[]
[]
[]
[]
["","","","","FTXN25MV1B9 / RXN25MV1B9","FTXN35MV1B9 / RXN35MV1B9","FTXN50MV1B9 / RXN50MV1B9","FTXN60MV1B9 / RXN60MV1B9"]
["Cooling capacity","Min.","","kW","1.300","1.300","1.630","1.750"]
["","Max.","","kW","3.000","3.800","6.200","6.500"]
["","Nom.","","kW","2.560","3.410","5.480","6.230"]
["Space cooling","SEER","","","5.61","5.61","5.61","5.15"]
["","Annual energy consumption","","kWh/a","160","213","342","423"]
["","Capacity","Pdesign","kW","2.56","3.41","5.48","6.23"]
["","Energy efficiency class","","","A+","A+","A+","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.51","2.58","3.64","3.80"]
["","SCOP/A","","","3.81","3.81","3.99","3.81"]
["","Energy efficiency class","","","A","A","A","A"]
["","Annual energy consumption","","kWh/a","922","948","1,277","1,396"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.70","15.90"]
["","Drain","OD","mm","16.5","16.5","16.5","16.5"]
["Nominal efficiency","EER","","","3.69 (1)","2.83 (1)","3.19 (1)","3.23 (1)"]
["","Annual energy consumption","","kWh","346.5","602.5","859","965.5"]
["","COP","","","4.06 (1)","3.77 (1)","3.75 (1)","3.81 (1)"]
["","Energy labeling Directive","Cooling","","A","C","B","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.840","3.580","5.620","6.400"]
["","Min.","","kW","1.300","1.300","1.170","1.200"]
["","Max.","","kW","4.000","4.750","6.600","7.100"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(2) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(2) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(2) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice.","(3) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(4) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]