{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-MB9"]
[]
[]
[]
[]
["","","","","FTXN25MV1B9","FTXN35MV1B9","FTXN50MV1B9","FTXN60MV1B9"]
["Sound pressure level","Heating","High","dBA","40","41","40","43"]
["","","Silent operation","dBA","21","22","32","33"]
["","","Low","dBA","29","30","35","37"]
["","Cooling","Silent operation","dBA","21","22","32","33"]
["","","Super high","dBA","41","42","44","46"]
["","","Low","dBA","29","30","35","37"]
["","","High","dBA","40","41","40","43"]
["","","Nom.","dBA","34","34","38","41"]
["","Cooling","Nom.","dBA","34","34","38","41"]
["Control systems","Infrared remote control","","","APGS02","APGS02","APGS02","APGS02"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.70","15.90"]
["","Drain","","","19.05","19.05","19.05","19.05"]
["Sound power level","Cooling","","dBA","53","54","55","61"]
["Dimensions","Unit","Width","mm","800","800","1,065","1,065"]
["","","Depth","mm","206","206","224","224"]
["","","Height","mm","288","288","310","310"]
["Casing","Colour","","","White","White","White","White"]
["Weight","Unit","","kg","9","9","14","14"]
["Power supply","Phase","","","1~","1~","1~","1~"]
["","Name","","","V1","V1","V1","V1"]
["","Frequency","","Hz","50","50","50","50"]
["","Voltage","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice."]