{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":78,"n_cols":7,"rows_kept":78,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXQ-A"]
[]
[]
[]
[]
["","","","","","FTXQ25AMV1B","FTXQ35AMV1B"]
["Sound pressure level","Heating","","High","dBA","","42.0"]
["","","","Medium","dBA","","35.0"]
["","","","Silent operation","dBA","","25.0"]
["","","","Low","dBA","","30.0"]
["","Cooling","","Medium","dBA","","35.0"]
["","","","Silent operation","dBA","","24.0"]
["","","","Low","dBA","","28.0"]
["","","","High","dBA","","41.0"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Infrared remote control","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Control systems","Infrared remote control","","","","","ARC470A1"]
["Piping connections","Liquid","","OD","mm","","6.35"]
["","Gas","","OD","mm","","9.50"]
["","Drain","","","","","18"]
["Power input","Cooling","","Nom.","kW","","0.025"]
["","Heating","","Nom.","kW","","0.031"]
["Sound power level","Cooling","","","dBA","","55"]
["Dimensions","Unit","","Width","mm","","770"]
["","","","Depth","mm","","232"]
["","","","Height","mm","","291"]
["Casing","Colour","","","","","White"]
["Weight","Unit","","","kg","","9.00"]
["Fan","Air flow rate","Heating","High","m³/min","","12.0"]
["","","","Medium","m³/min","","10.0"]
["","","","Low","m³/min","","8.3"]
["","","","Silent operation","m³/min","","6.9"]
["","","Cooling","Low","m³/min","","7.0"]
["","","","Medium","m³/min","","8.5"]
["","","","High","m³/min","","10.5"]
["","","","Silent operation","m³/min","","6.0"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["Power input","Cooling","","Nom.","kW","0.023"]
["","Heating","","Nom.","kW","0.027"]
["Casing","Colour","","","","White"]
["Dimensions","Unit","","Height","mm","291"]
["","","","Width","mm","770"]
["","","","Depth","mm","232"]
["Weight","Unit","","","kg","9"]
["Fan","Air flow rate","Cooling","High","m³/min","10.2"]
["","","","Medium","m³/min","8.1"]
["","","","Low","m³/min","6.5"]
["","","","Silent operation","m³/min","5"]
["","","Heating","High","m³/min","11.1"]
["","","","Medium","m³/min","9.6"]
["","","","Low","m³/min","8.1"]
["","","","Silent operation","m³/min","6.8"]
["Sound power level","Cooling","","","dBA","55"]
["Sound pressure level","Cooling","","High","dBA","40"]
["","","","Medium","dBA","34"]
["","","","Low","dBA","26"]
["","","","Silent operation","dBA","23"]
["","Heating","","High","dBA","40"]
["","","","Medium","dBA","34"]
["","","","Low","dBA","29"]
["","","","Silent operation","dBA","25"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.5"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC470A1"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]