{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-DL"]
[]
[]
[]
[]
["","","","","","FTXTA30D2V1BL"]
["Power input","Cooling","","Nom.","kW","0.023"]
["","Heating","","Nom.","kW","0.022"]
["Casing","Colour","","","","Casing: Black, Panel: Dark brown leather "]
["Dimensions","Unit","","Height","mm","295"]
["","","","Width","mm","798"]
["","","","Depth","mm","189"]
["Weight","Unit","","","kg","12"]
["Fan","Air flow rate","Cooling","High","m³/min","13.1"]
["","","","Medium","m³/min","9.0"]
["","","","Low","m³/min","6.0"]
["","","","Silent operation","m³/min","4.9"]
["","","Heating","High","m³/min","12.3"]
["","","","Medium","m³/min","8.2"]
["","","","Low","m³/min","5.8"]
["","","","Silent operation","m³/min","5.0"]
["Sound power level","Cooling","","","dBA","60"]
["","Heating","","","dBA","60"]
["Sound pressure level","Cooling","","High","dBA","43"]
["","","","Medium","dBA","32"]
["","","","Low","dBA","25"]
["","","","Silent operation","dBA","20"]
["","Heating","","High","dBA","41"]
["","","","Medium","dBA","31"]
["","","","Low","dBA","24"]
["","","","Silent operation","dBA","19"]
["Refrigerant","GWP","","","","675.0"]
["Piping connections","Liquid","","OD","mm","6.35"]
["","Gas","","OD","mm","9.50"]
["","Drain","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A95"]
["","Wired remote control","","","","BRC073A1"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Energy Efficiency Range","","","","","A+++ ~ D"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","","(3) - See separate drawing for electrical data"]