{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Power input","Cooling","","Nom.","kW","0.032","0.037"]
["","Heating","","Nom.","kW","0.037","0.04"]
["Casing","Colour","","","","White","White"]
["Dimensions","Unit","","Height","mm","294","300"]
["","","","Width","mm","811","1040"]
["","","","Depth","mm","272","295"]
["Weight","Unit","","","kg","10","14.5"]
["Fan","Air flow rate","Cooling","High","m³/min","11.7","15.5"]
["","","","Medium","m³/min","8","9.2"]
["","","","Low","m³/min","6.3","5.7"]
["","","","Silent operation","m³/min","5.2","4.6"]
["","","Heating","High","m³/min","12.2","17.7"]
["","","","Medium","m³/min","7.5","11"]
["","","","Low","m³/min","5.1","7.5"]
["","","","Silent operation","m³/min","4.1","6.3"]
["Sound power level","Cooling","","","dBA","60","60"]
["","Heating","","","dBA","61","61"]
["Sound pressure level","Cooling","","High","dBA","45","46"]
["","","","Medium","dBA","33","32"]
["","","","Low","dBA","25","24"]
["","","","Silent operation","dBA","21","20"]
["","Heating","","High","dBA","45","46"]
["","","","Medium","dBA","31","31"]
["","","","Low","dBA","22","22"]
["","","","Silent operation","dBA","19","19"]
["Piping connections","Liquid","","OD","mm","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5"]
["","Drain","","","","16 (inner diameter of connecting hose)","16 (inner diameter of connecting hose)"]
["Control systems","Infrared remote control","","","","ARC466A55","ARC466A55"]
["","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Power supply","Name","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]