{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":12,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXAQ-P"]
[]
[]
[]
[]
["","","","","","FXAQ15PAV1","FXAQ20PAV1","FXAQ25PAV1","FXAQ32PAV1","FXAQ40PAV1","FXAQ50PAV1","FXAQ63PAV1"]
["Standard Accessories","Installation and operation manual","","","","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual"]
["","Installation panel","","","","Installation panel","Installation panel","Installation panel","Installation panel","Installation panel","Installation panel","Installation panel"]
["","Paper pattern for installation","","","","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation","Paper pattern for installation"]
["","Insulation tape","","","","Insulation tape","Insulation tape","Insulation tape","Insulation tape","Insulation tape","Insulation tape","Insulation tape"]
["","Clamps","","","","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps","Clamps"]
["","Screws","","","","Screws","Screws","Screws","Screws","Screws","Screws","Screws"]
["Refrigerant","Type","","","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","GWP","","","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Piping connections","Liquid","","OD","mm","","","6.35","6.35","6.35","6.35","9.52"]
["","","","Type","","","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","","","12.7","12.7","12.7","12.7","15.9"]
["","","","Type","","","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Dimensions","Unit","","Width","mm","","","795","795","1,050","1,050","1,050"]
["","","","Depth","mm","","","238","238","238","238","238"]
["","","","Height","mm","","","290","290","290","290","290"]
["Casing","Colour","","","","","","White (3.0Y8.5/0.5)","White (3.0Y8.5/0.5)","White (3.0Y8.5/0.5)","White (3.0Y8.5/0.5)","White (3.0Y8.5/0.5)"]
["Weight","Unit","","","kg","","","11","11","14","14","14"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","","","16","16","16","16","16"]
["Power supply","Phase","","","","","","1~","1~","1~","1~","1~"]
["","Name","","","","","","V1","V1","V1","V1","V1"]
["","Frequency","","","Hz","","","50","50","50","50","50"]
["","Voltage","","","V","","","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m (horizontal)"]
["","","","","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","","","","(4) - Sound levels are measured in an anechoic room.","(4) - Sound levels are measured in an anechoic room.","(4) - Sound levels are measured in an anechoic room.","(4) - Sound levels are measured in an anechoic room.","(4) - Sound levels are measured in an anechoic room."]
["","","","","","","","(5) - Operation sound differs with operation and ambient conditions","(5) - Operation sound differs with operation and ambient conditions","(5) - Operation sound differs with operation and ambient conditions","(5) - Operation sound differs with operation and ambient conditions","(5) - Operation sound differs with operation and ambient conditions"]
["","","","","","","","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit.","(6) - The sound pressure level is measured via a microphone at 1m distance of the unit."]
["","","","","","","","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","","","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","","","(9) - MCA/MFA: MCA = 1.25 x FLA","(9) - MCA/MFA: MCA = 1.25 x FLA","(9) - MCA/MFA: MCA = 1.25 x FLA","(9) - MCA/MFA: MCA = 1.25 x FLA","(9) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","","","","(10) - MFA ≤ 4 x FLA","(10) - MFA ≤ 4 x FLA","(10) - MFA ≤ 4 x FLA","(10) - MFA ≤ 4 x FLA","(10) - MFA ≤ 4 x FLA"]
["","","","","","","","(11) - Next lower standard fuse rating minimum 16A","(11) - Next lower standard fuse rating minimum 16A","(11) - Next lower standard fuse rating minimum 16A","(11) - Next lower standard fuse rating minimum 16A","(11) - Next lower standard fuse rating minimum 16A"]
["","","","","","","","(12) - Select wire size based on the value of MCA","(12) - Select wire size based on the value of MCA","(12) - Select wire size based on the value of MCA","(12) - Select wire size based on the value of MCA","(12) - Select wire size based on the value of MCA"]
["","","","","","","","(13) - Instead of a fuse, use a circuit breaker","(13) - Instead of a fuse, use a circuit breaker","(13) - Instead of a fuse, use a circuit breaker","(13) - Instead of a fuse, use a circuit breaker","(13) - Instead of a fuse, use a circuit breaker"]
["","","","","","","","(14) - Contains fluorinated greenhouse gases","(14) - Contains fluorinated greenhouse gases","(14) - Contains fluorinated greenhouse gases","(14) - Contains fluorinated greenhouse gases","(14) - Contains fluorinated greenhouse gases"]
["Cooling capacity","Total capacity","","At high fan speed","kW","1.7 (1)","2.2 (1)"]
["Heating capacity","Total capacity","","At high fan speed","kW","1.9 (2)","2.5 (2)"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.025","0.029"]
["","Heating","","At high fan speed","kW","0.025","0.029"]
["Dimensions","Unit","","Height","mm","290","290"]
["","","","Width","mm","795","795"]
["","","","Depth","mm","238","238"]
["Weight","Unit","","","kg","11","11"]
["Casing","Colour","","","","White (3.0Y8.5/0.5)","White (3.0Y8.5/0.5)"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","7.0","7.5"]
["","","","At low fan speed","m³/min","4.5","4.5"]
["Refrigerant","GWP","","","","2087.5","2087.5"]
["Sound power level","Cooling","","At high fan speed","dBA","52.0","53.0"]
["Sound pressure level","Cooling","","At high fan speed","dBA","34.0","35.0"]
["","","","At low fan speed","dBA","29.0","29.0"]
["Piping connections","Liquid","","Type","","Flare connection","Flare connection"]
["","","","OD","mm","6.35","6.35"]
["","Gas","","Type","","Flare connection","Flare connection"]
["","","","OD","mm","12.7","12.7"]
["Air filter","Type","","","","Washable resin net","Washable resin net"]
["Power supply","Frequency","","","Hz","50","50"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","16","16"]