{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":61,"n_cols":13,"rows_kept":61,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXDA-A"]
[]
[]
[]
[]
["","","","","","FXDA10A2VEB","FXDA15A2VEB","FXDA20A2VEB","FXDA25A2VEB","FXDA32A2VEB","FXDA40A2VEB","FXDA63A2VEB","FXDA50A2VEB"]
["Sound pressure level","Heating","","At high fan speed","dBA","29.0","32.0","33.0","33.0","33.0","34.0","36.0","35.0"]
["","","","At low fan speed","dBA","26.0","27.0","27.0","27.0","27.0","28.0","30.0","29.0"]
["","","","At medium fan speed","dBA","28.0","31.0","31.0","31.0","31.0","32.0","34.0","33.0"]
["","Cooling","","At low fan speed","dBA","26.0","27.0","27.0","27.0","27.0","28.0","30.0","29.0"]
["","","","At high fan speed","dBA","29.0","32.0","33.0","33.0","33.0","34.0","36.0","35.0"]
["","","","At medium fan speed","dBA","28.0","31.0","31.0","31.0","31.0","32.0","34.0","33.0"]
["Standard Accessories","Installation and operation manual","","","","1","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1","1"]
["","Sealing material (drain hose)","","","","2","2","2","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8","8"]
["","Screws","","","","26","26","26","26","26","26","26","26"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2","2"]
["","Sealing material","","","","2","2","2","2","2","2","2","2"]
["","Clamps","","","","12","12","12","12","12","12","12","12"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.026 (1)","0.035 (1)","0.030 (1)","0.030 (1)","0.035 (1)","0.038 (1)","0.058 (1)","0.049 (1)"]
["","Heating","","At high fan speed","kW","0.026 (1)","0.035 (1)","0.030 (1)","0.030 (1)","0.035 (1)","0.038 (1)","0.058 (1)","0.049 (1)"]
["Cooling capacity","Total capacity","","At high fan speed","kW","1.10","1.70","2.20","2.80","3.60","4.50","7.10","5.60"]
["Piping connections","Liquid","","OD","mm","6","6","6","6","6","6","6","6"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","9.52","9.52","9.52","9.52","9.52","12.70","12.70","12.70"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Required ceiling void >","mm","","","","240","240","240","240","240","240","240","240"]
["Sound power level","Cooling","","At high fan speed","dBA","48","50","51","51","51","52","54","53"]
["Air filter","Type","","","","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable"]
["Dimensions","Unit","","Width","mm","750","750","750","750","750","950","1,150","950"]
["","","","Depth","mm","620","620","620","620","620","620","620","620"]
["","","","Height","mm","200","200","200","200","200","200","200","200"]
["Casing","Material","","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["","Colour","","","","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)"]
["Weight","Unit","","","kg","22.0","22.0","23.0","23.0","23.0","26.5","30.5","26.5"]
["Fan","External static pressure - 50Hz","","High","Pa","30","30","30","30","30","44","44","44"]
["","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","5.2","6.5","8.0","8.0","8.0","10.5","16.5","12.5"]
["","","","At low fan speed","m³/min","4.7","5.8","6.4","6.4","6.4","8.5","13.0","10.0"]
["Drain-up height","mm","","","","600","600","600","600","600","600","600","600"]
["Heating capacity","Total capacity","","At high fan speed","kW","1.30","1.90","2.50","3.20","4.00","5.00","8.00","6.30"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6","6","6","6","6","6","6"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","","VE","VE","VE","VE","VE","VE","VE","VE"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting.","(1) - Values are valid for the factory setting."]
["","","","","","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(2) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(3) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(4) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(5) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)"]
["","","","","","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA","(8) - MCA/MFA: MCA = 1.1 x FLA"]
["","","","","","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker","(9) - Instead of a fuse, use a circuit breaker"]
["","","","","","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA","(10) - Select wire size based on the value of MCA"]
["","","","","","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases"]