{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXDQ-M9"]
[]
[]
[]
[]
["","","","","FXDQ20M9V3B9","FXDQ25M9V3B9"]
["Refrigerant","Type","","","R-410A","R-410A"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","","Type","","Flare connection","Flare connection"]
["","Gas","OD","mm","12.7","12.7"]
["","","Type","","Flare connection","Flare connection"]
["","Drain","","","I.D. 21.6, O.D. 27.2","I.D. 21.6, O.D. 27.2"]
["Required ceiling void >","mm","","","250","250"]
["Dimensions","Unit","Width","mm","502","502"]
["","","Depth","mm","652","652"]
["","","Height","mm","230","230"]
["Casing","Material","","","Galvanised steel","Galvanised steel"]
["","Colour","","","Unpainted","Unpainted"]
["Weight","Unit","","kg","17","17"]
["Current - 50Hz","Maximum fuse amps (MFA)","","A","16","16"]
["Power supply","Phase","","","1~","1~"]
["","Name","","","V1","V1"]
["","Frequency","","Hz","50","50"]
["","Voltage","","V","230","230"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]