{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXDQ-P2"]
[]
[]
[]
[]
["","","","","FXDQ15P2VE","FXDQ20P2VE","FXDQ25P2VE","FXDQ32P2VE","FXDQ40P2VE","FXDQ50P2VE","FXDQ63P2VE"]
["Refrigerant","Type","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Cooling capacity","Nom.","","kW","1.70","2.20","2.80","3.60","4.50","5.60","7.10"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","9.52"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","OD","mm","12.7","12.7","12.7","12.7","12.7","12.7","15.9"]
["","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Required ceiling void >","mm","","","240","240","240","240","240","240","240"]
["Dimensions","Unit","Width","mm","750","750","750","750","950","950","1,150"]
["","","Depth","mm","620","620","620","620","620","620","620"]
["","","Height","mm","200","200","200","200","200","200","200"]
["Casing","Material","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["","Colour","","","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)","Not painted (galvanised)"]
["Weight","Unit","","kg","22.0","22.0","22.0","22.0","26.0","26.0","29.0"]
["Fan","External static pressure - 50Hz","High","Pa","30.0","30.0","30.0","30.0","44.0","44.0","44.0"]
["","External static pressure - 60Hz","High","Pa","30","30","30","30","44","44","44"]
["Drain-up height","mm","","","600","600","600","600","600","600","600"]
["Heating capacity","Nom.","","kW","1.90","2.50","3.20","4.00","5.00","6.30","8.00"]
["Current - 50Hz","Maximum fuse amps (MFA)","","A","16","16","16","16","16","16","16"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","VE","VE","VE","VE","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m; level difference: 0m"]
["","","","","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat.","(3) - Capacities are net, including a deduction for cooling (an addition for heating) for indoor fan motor heat."]
["","","","","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)","(4) - External static pressure is changeable to set by the remote control (from standard to high, see installation manual)"]
["","","","","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction.","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction.","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction.","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction.","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction.","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction.","(5) - The operation sound levels are conversion values in anechoic chamber. In practice, sound levels tend to be higher than the specified values due to ambient noise or reflection. The sound level will increase by ± 5dBA when the suction place is changed to bottom suction."]
["","","","","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(6) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%.","(7) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(8) - MCA/MFA: MCA = 1.25 x FLA","(8) - MCA/MFA: MCA = 1.25 x FLA","(8) - MCA/MFA: MCA = 1.25 x FLA","(8) - MCA/MFA: MCA = 1.25 x FLA","(8) - MCA/MFA: MCA = 1.25 x FLA","(8) - MCA/MFA: MCA = 1.25 x FLA","(8) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","(9) - MFA ≤ 4 x FLA","(9) - MFA ≤ 4 x FLA","(9) - MFA ≤ 4 x FLA","(9) - MFA ≤ 4 x FLA","(9) - MFA ≤ 4 x FLA","(9) - MFA ≤ 4 x FLA","(9) - MFA ≤ 4 x FLA"]
["","","","","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker","(10) - Instead of a fuse, use a circuit breaker"]
["","","","","(11) - Select wire size based on the value of MCA","(11) - Select wire size based on the value of MCA","(11) - Select wire size based on the value of MCA","(11) - Select wire size based on the value of MCA","(11) - Select wire size based on the value of MCA","(11) - Select wire size based on the value of MCA","(11) - Select wire size based on the value of MCA"]
["","","","","(12) - Next lower standard fuse rating minimum 15A","(12) - Next lower standard fuse rating minimum 15A","(12) - Next lower standard fuse rating minimum 15A","(12) - Next lower standard fuse rating minimum 15A","(12) - Next lower standard fuse rating minimum 15A","(12) - Next lower standard fuse rating minimum 15A","(12) - Next lower standard fuse rating minimum 15A"]