{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":14,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXFQ-A"]
[]
[]
[]
[]
["","","","","","FXFQ20AVEB","FXFQ25AVEB","FXFQ32AVEB","FXFQ40AVEB","FXFQ50AVEB","FXFQ63AVEB","FXFQ80AVEB","FXFQ100AVEB","FXFQ125AVEB"]
["Sound pressure level","Heating","","At high fan speed","dBA","","","","","","35.0"]
["","","","At low fan speed","dBA","","","","","","30.0"]
["","","","At medium fan speed","dBA","","","","","","33.0"]
["","Cooling","","At low fan speed","dBA","","","","","","30.0"]
["","","","At high fan speed","dBA","","","","","","35.0"]
["","","","At medium fan speed","dBA","","","","","","33.0"]
["Standard Accessories","Operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Clamp for drain hose","","","","1","1","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","1","1","1","1","1","1","1","1","1"]
["","Screws","","","","1","1","1","1","1","1","1","1","1"]
["","Installation guide","","","","1","1","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2","2","2"]
["","Sealing pads","","","","4","4","4","4","4","4","4","4","4"]
["","Drain sealing pad","","","","1","1","1","1","1","1","1","1","1"]
["","Clamps","","","","1","1","1","1","1","1","1","1","1"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","","2,087.5","2,087.5","2,087.5"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","","","","","","0.06"]
["","Heating","","At high fan speed","kW","","","","","","0.06"]
["Cooling capacity","Total capacity","","At high fan speed","kW","","","","","","7.10"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","12.70","12.70","12.70","12.70","12.70","15.90","15.90","15.90","15.90"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)","VP25 (O.D. 32 / I.D. 25)"]
["Decoration panel 4","Dimensions","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["","","","Width","mm","950","950","950","950","950","950","950","950","950"]
["","","","Height","mm","50","50","50","50","50","50","50","50","50"]
["","Model","","","","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers","BYCQ140D7W1 - white with grey louvers"]
["","Colour","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["","Weight","","","kg","5.4","5.4","5.4","5.4","5.4","5.4","5.4","5.4","5.4"]
["Sound power level","Cooling","","At high fan speed","dBA","","","","","","53"]
["Dimensions","Unit","","Width","mm","840","840","840","840","840","840","840","840","840"]
["","","","Depth","mm","840","840","840","840","840","840","840","840","840"]
["","","","Height","mm","204","204","204","204","204","204","246","246","288"]
["Casing","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate"]
["Weight","Unit","","","kg","19","19","19","20","21","21","24","24","26"]
["Decoration panel 2","Weight","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["","Model","","","","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel","BYCQ140D7GW1 - auto cleaning panel"]
["","Dimensions","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["","","","Width","mm","950","950","950","950","950","950","950","950","950"]
["","","","Height","mm","130","130","130","130","130","130","130","130","130"]
["","Colour","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Decoration panel 3","Dimensions","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["","","","Height","mm","50","50","50","50","50","50","50","50","50"]
["","","","Width","mm","950","950","950","950","950","950","950","950","950"]
["","Colour","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["","Model","","","","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white","BYCQ140D7W1W - full white"]
["","Weight","","","kg","5.4","5.4","5.4","5.4","5.4","5.4","5.4","5.4","5.4"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","","","","","","16.5"]
["","","","At low fan speed","m³/min","","","","","","10.5"]
["Decoration panel","Weight","","","kg","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3","10.3"]
["","Model","","","","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter","BYCQ140D7GFW1 - auto cleaning panel with fine mesh filter"]
["","Dimensions","","Height","mm","130","130","130","130","130","130","130","130","130"]
["","","","Depth","mm","950","950","950","950","950","950","950","950","950"]
["","","","Width","mm","950","950","950","950","950","950","950","950","950"]
["","Colour","","","","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)","Pure White (RAL 9010)"]
["Heating capacity","Total capacity","","At high fan speed","kW","","","","","","8.0"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","16","16","16","16","16","16","16","16","16"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","","VE","VE","VE","VE","VE","VE","VE","VE","VE"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt.","(3) - The BYCQ140D7W1W has white insulations. Be informed that formation of dirt on white insulation is visibly stronger and that it is consequently not advised to install the BYCQ140D7W1W decoration panel in environments exposed to concentrations of dirt."]
["","","","","","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates.","(4) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(5) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%.","(6) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA","(7) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA","(8) - MFA ≤ 4 x FLA"]
["","","","","","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A","(9) - Next lower standard fuse rating minimum 16A"]
["","","","","","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases","(10) - Contains fluorinated greenhouse gases"]
["","","","","","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel.","(11) - BYCQ140D7W1: pure white standard panel with grey louvers; BYCQ140D7W1W: pure white standard panel with white louvers; BYCQ140D7GW1: pure white auto cleaning panel."]
["","","","","","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker","(12) - Instead of a fuse, use a circuit breaker"]
["","","","","","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA","(13) - Select wire size based on the value of MCA"]
["","","","","","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB","(14) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp.: 48°CDB"]
["Refrigerant","GWP","","","","","","","","","2,087.5"]
["Air filter","Type","","","","","","","","","Resin net"]