{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":13,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXHQ-A"]
[]
[]
[]
[]
["","","","","","FXHQ32AVEB8","FXHQ63AVEB8","FXHQ100AVEB8","FXHQ32AVEB9 (Archived)","FXHQ63AVEB (Archived)","FXHQ63AVEB9 (Archived)","FXHQ100AVEB (Archived)","FXHQ100AVEB9 (Archived)"]
["Sound pressure level","Heating","","At high fan speed","dBA","36.0","37.0","44.0","36.0","37.0","37.0","44.0","44.0"]
["","","","At low fan speed","dBA","31.0","34.0","34.0","31.0","34.0","34.0","34.0","34.0"]
["","","","At medium fan speed","dBA","34.0","35.0","37.0","34.0","35.0","35.0","37.0","37.0"]
["","Cooling","","At low fan speed","dBA","31.0","34.0","34.0","31.0","34.0","34.0","34.0","34.0"]
["","","","At high fan speed","dBA","36.0","37.0","44.0","36.0","37.0","37.0","44.0","44.0"]
["","","","At medium fan speed","dBA","34.0","35.0","37.0","34.0","35.0","35.0","37.0","37.0"]
["Standard Accessories","Operation manual","","","","","","","Operation manual","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Installation manual","","","","","","","Installation manual","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Declaration of conformity","","","","","","","Declaration of conformity","Declaration of conformity","Declaration of conformity","Declaration of conformity","Declaration of conformity"]
["","Drain hose","","","","1","1","1","Drain hose","Drain hose","Drain hose","Drain hose","Drain hose"]
["","Clamp metal","","","","","","","Clamp metal","Clamp metal","Clamp metal","Clamp metal","Clamp metal"]
["","Washer for hanger bracket","","","","","","","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket","Washer for hanger bracket"]
["","Clamps","","","","","","","Clamps","Clamps","Clamps","Clamps","Clamps"]
["","Joint insulating material","","","","","","","Joint insulating material","Joint insulating material","Joint insulating material","Joint insulating material","Joint insulating material"]
["","Sealing material","","","","6","6","6","Sealing material","Sealing material","Sealing material","Sealing material","Sealing material"]
["","Installation pattern","","","","","","","Installation pattern","Installation pattern","Installation pattern","Installation pattern","Installation pattern"]
["","Resin bushing","","","","1","1","1","Resin bushing","Resin bushing","Resin bushing","Resin bushing","Resin bushing"]
["","Wiring fixture","","","","2","2","2","Wiring fixture","Wiring fixture","Wiring fixture","Wiring fixture","Wiring fixture"]
["","Screw for wiring fixture","","","","","","","Screw for wiring fixture","Screw for wiring fixture","Screw for wiring fixture","Screw for wiring fixture","Screw for wiring fixture"]
["Refrigerant","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.107","0.111","0.237","0.107","0.111","0.111","0.237","0.237"]
["","Heating","","At high fan speed","kW","0.107","0.111","0.237","0.107","0.111","0.111","0.237","0.237"]
["Cooling capacity","Total capacity","","At high fan speed","kW","3.6","7.1","11.2","3.6","7.1","7.1","11.2","11.2"]
["Piping connections","Liquid","","OD","mm","6.35","9.52","9.52","6.4","9.52","9.5","9.52","9.5"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","12.7","15.9","15.9","12.7","15.9","15.9","15.9","15.9"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","","VP20","VP20","VP20","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Cooling","","At high fan speed","dBA","54.0","55.0","62.0","54","55","55","62","62"]
["Air filter","Type","","","","Resin net","Resin net","Resin net","Resin net with mold resistance","Resin net with mold resistance","Resin net with mold resistance","Resin net with mold resistance","Resin net with mold resistance"]
["Dimensions","Unit","","Width","mm","960","1,270","1,590","960","1,270","1,270","1,590","1,590"]
["","","","Depth","mm","690","690","690","690","690","690","690","690"]
["","","","Height","mm","235","235","235","235","235","235","235","235"]
["Casing","Material","","","","Resin, sheet metal","Resin, sheet metal","Resin, sheet metal","Resin","Resin","Resin","Resin","Resin"]
["","Colour","","","","Fresh White","Fresh White","Fresh White","Fresh White","Fresh White","Fresh White","Fresh White","Fresh White"]
["Weight","Unit","","","kg","27","35","42","24","33","33","39","39"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","14.0","20.0","29.5","14.0","20.0","20.0","29.5","29.5"]
["","","","At low fan speed","m³/min","10.0","14.0","19.0","10.0","14.0","14.0","19.0","19.0"]
["Heating capacity","Total capacity","","At high fan speed","kW","4.0","8.0","12.5","4.0","8.0","8.0","12.5","12.5"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","16","16","16","16","16","16","16","16"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","","","","","VE","VE","VE","VE","VE"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50","50/60","50","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240","220-240/220","220-240","220-240/220"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(1) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(1) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(1) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(1) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Maximum allowable voltage range variation between phases is 2%.","(2) - Maximum allowable voltage range variation between phases is 2%.","(2) - Maximum allowable voltage range variation between phases is 2%.","(2) - Maximum allowable voltage range variation between phases is 2%.","(2) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - MCA/MFA: MCA = 1.25 x FLA","(3) - MCA/MFA: MCA = 1.25 x FLA","(3) - MCA/MFA: MCA = 1.25 x FLA","(3) - MCA/MFA: MCA = 1.25 x FLA","(3) - MCA/MFA: MCA = 1.25 x FLA"]
["","","","","","(4) - Instead of a fuse, use a circuit breaker","(4) - Instead of a fuse, use a circuit breaker","(4) - Instead of a fuse, use a circuit breaker","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA","(4) - MFA ≤ 4 x FLA"]
["","","","","","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Select wire size based on the value of MCA","(5) - Next lower standard fuse rating minimum 16A","(5) - Next lower standard fuse rating minimum 16A","(5) - Next lower standard fuse rating minimum 16A","(5) - Next lower standard fuse rating minimum 16A","(5) - Next lower standard fuse rating minimum 16A"]
["","","","","","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Contains fluorinated greenhouse gases","(6) - Select wire size based on the value of MCA","(6) - Select wire size based on the value of MCA","(6) - Select wire size based on the value of MCA","(6) - Select wire size based on the value of MCA","(6) - Select wire size based on the value of MCA"]
["","","","","","","","","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker"]
["","","","","","","","","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases","(8) - Contains fluorinated greenhouse gases"]
["Standard Accessories","Thermal insulation tube","","","","2","2","2"]
["","Wire clamp material","","","","7","7","7"]
["","Hose band","","","","1","1","1"]
["","Screws","","","","2","2","2"]
["","Washer","","","","8","8","8"]
["","General safety precautions","","","","1","1","1"]
["","Installation and operation manual","","","","1","1","1"]
["","Paper pattern for installation","","","","1","1","1"]