{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":5,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-P7H"]
[]
[]
[]
[]
["","","","","FXMQ50P7VEH"]
["Refrigerant","Type","","","R-410A"]
["Cooling capacity","Nom.","","kW","5.6 (1)"]
["Piping connections","Liquid","OD","mm","6.35"]
["","","Type","","Flare connection"]
["","Gas","OD","mm","12.7"]
["","","Type","","Flare connection"]
["","Drain","","","VP25 (I.D. 25/O.D. 32)"]
["Required ceiling void >","mm","","","350"]
["Dimensions","Unit","Width","mm","1,000"]
["","","Depth","mm","700"]
["","","Height","mm","300"]
["Casing","Material","","","Galvanised steel plate"]
["","Colour","","","Unpainted"]
["Weight","Unit","","kg","35"]
["Fan","External static pressure - 50Hz","High","Pa","200"]
["","External static pressure - 60Hz","High","Pa","200"]
["Drain-up height","mm","","","625"]
["Decoration panel","Weight","","kg","4.5"]
["","Model","","","BYBS71DJW1"]
["","Dimensions","Height","mm","55"]
["","","Depth","mm","500"]
["","","Width","mm","1,100"]
["","Colour","","","White (10Y9/0.5)"]
["Heating capacity","Nom.","","kW","6.3 (2)"]
["Current - 50Hz","Maximum fuse amps (MFA)","","A","16"]
["Power supply","Phase","","","1~"]
["","Name","","","VE"]
["","Frequency","","Hz","50/60"]
["","Voltage","","V","220-240/220 +/-10%"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]