{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HXHD-A8"]
[]
[]
[]
[]
["","","","","","HXHD125A8V1B","HXHD200A8Y1B"]
["Casing","Colour","","","","Metallic grey","Metallic grey"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","705","705"]
["","","","Width","mm","600","600"]
["","","","Depth","mm","695","695"]
["Weight","Unit","","","kg","92","147"]
["Refrigerant","Type","","","","R-134a","R-134a"]
["","Charge","","","kg","2","2.6"]
["Sound power level","Nom.","","","dBA","55","60"]
["Sound pressure level","Nom.","","","dBA","42, 43","46, 46"]
["Operation range","Heating","Water side","Min.","°C","25","25"]
["","","","Max.","°C","80.0","80.0"]
["Power supply","Phase","","","","1~","3~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","380-415"]
["Current","Recommended fuses","","","A","20","16"]
["Notes","","","","","(1) - EW 40°C; LW 45°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB","(1) - EW 40°C; LW 45°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB"]
["","","","","","(2) - For water Dt 5°C","(2) - For water Dt 10°C"]
["","","","","","(3) - Sound levels are measured at: EW 55°C; LW 65°C","(3) - Sound levels are measured at: EW 55°C; LW 65°C"]
["","","","","","(4) - Sound levels are measured at: EW 70°C; LW 80°C","(4) - Sound levels are measured at: EW 70°C; LW 80°C"]
["","","","","","(5) - Field setting","(5) - Field setting"]
["","","","","","(6) - In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax","(6) - In accordance with EN/IEC 61000-3-11, it may be necessary to consult the distribution network operator to ensure that the equipment is connected only to a supply with Zsys (system impedance) ≤ Zmax"]
["","","","","","(7) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A.","(7) - European/International Technical Standard setting the limits for voltage changes, voltage fluctuations and flicker in public low-voltage supply systems for equipment with rated current ≤ 75A."]
["","","","","","(8) - Zsys: system impedance","(8) - Zsys: system impedance"]
["","","","","","(9) - Short-circuit power","(9) - Short-circuit power"]