{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LREQ-BY1R"]
[]
[]
[]
[]
["","","","","","LREQ15BY1R","LREQ20BY1R"]
["Operation range","Ambient temperature","","Min.","°C","-20 (2)","-20 (2)"]
["","","","Max.","°C","43","43"]
["","Evaporator","Cooling","Min.","°CDB","-45 (1)","-45 (1)"]
["","","","Max.","°CDB","10","10"]
["Compressor 2","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Fan motor 2","Output","","","W","350","750"]
["Fan","Quantity","","","","2","2"]
["","Type","","","","Propeller fan","Propeller fan"]
["","Air flow rate","Cooling","Nom.","m³/min","230","240"]
["Fan motor","Output","","","W","350","750"]
["Dimensions","Unit","","Height","mm","1680","1680"]
["","","","Width","mm","1240","1240"]
["","","","Depth","mm","765","765"]
["Weight","Unit","","","kg","331","337"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["Casing","Colour","","","","Ivory white (Munsell code: 5Y7.5/1)","Ivory white (Munsell code: 5Y7.5/1)"]
["Refrigerant","GWP","","","","2087.5","2087.5"]
["Heat exchanger","Type","","","","Cross fin coil","Cross fin coil"]
["Refrigerant","Charge","","","kg","11.5","11.5"]
["","Charge","","","tCO2Eq","24.0","24.0"]
["Power supply","Phase","","","","3~","3~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","380-415","380-415"]
["Current","Nominal running current (RLA) - 50Hz","Compressor 2","Cooling","A","8.2","8.4"]
["","","Compressor 1","Cooling","A","7.0","9.5"]
["","","Compressor 3","Cooling","A","8.2","8.4"]
["Notes","","","","","(1) - When target evaporating temperature is -20°C or lower, there is the possibility to add the refrigerant oil. If the refrigerant oil is added, the target evaporating temperature can not change to -20°C or higher.","(1) - When target evaporating temperature is -20°C or lower, there is the possibility to add the refrigerant oil. If the refrigerant oil is added, the target evaporating temperature can not change to -20°C or higher."]
["","","","","","(2) - In the usage environment which outdoor temperature becomes lower than -10°C, installation of windbreak board or snowbreak hood is needed. For details, see the service manual.","(2) - In the usage environment which outdoor temperature becomes lower than -10°C, installation of windbreak board or snowbreak hood is needed. For details, see the service manual."]
["","","","","","(3) - Compressor 2 and 3","(3) - Compressor 2 and 3"]