{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","NHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","NHY2KOMB28AA","NHY2KOMB32AA"]
["Gas","Connection","","Diameter","mm","15","15"]
["","Consumption (G20)","","Min","m³/h","0.74","0.79"]
["","","","Max","m³/h","3.02","3.39"]
["","Consumption (G25)","","Min","m³/h","0.84","0.89"]
["","","","Max","m³/h","3.46","3.92"]
["","Consumption (G31)","","Min","m³/h","0.28","0.30"]
["","","","Max","m³/h","1.15","1.29"]
["","NOx class","","","","6","6"]
["Central heating","Heat input Qn (net calorific value)","Nom","Min","kW","7.1","7.6"]
["","","","Max","kW","23.7","27.0"]
["","Heat input Qn (gross calorific value)","Nom","Min","kW","8.0","8.3"]
["","","","Max","kW","26.3","30.0"]
["","Output Pn at 80/60°C","","Min","kW","7.1","7.4"]
["","","","Nom","kW","23.1","26.6"]
["","Output Pnc at 50/30°C","","Min","kW","7.7","8.2"]
["","","","Nom","kW","25.4","28.9"]
["Domestic hot water","Heat input (net calorific value) Qnw","Nom","Min","kW","7.2","7.6"]
["","","","Max","kW","29.1","32.7"]
["","Heat input (gross calorific value) Qnw","Nom","Min","kW","7.9","8.4"]
["","","","Max","kW","32.3","36.2"]
["","Efficiency","","Nom","%","105","105"]
["Supply air","Connection","","","mm","100","100"]
["","Concentric","","","","Yes","Yes"]
["Flue gas","Connection","","","mm","60","60"]
["Casing","Colour","","","","White - RAL9010","White - RAL9010"]
["","Material","","","","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","Height","Casing","mm","650","710"]
["","","","Width","mm","450","450"]
["","","","Depth","mm","240","240"]
["Weight","Unit","","Full","kg","33","36"]
["Domestic hot water heating","General","","Declared load profile","","XL","XL"]
["","","","Water heating energy efficiency class","","A","A"]
["Space heating","General","","Seasonal space heating eff. class","","A","A"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - 80/60","(1) - 80/60"]
["","","","","","(2) - Setpoint 60°C","(2) - Setpoint 60°C"]
["","","","","","(3) - Setpoint 40°C","(3) - Setpoint 40°C"]