{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":8,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-K1"]
[]
[]
[]
[]
["","","","","","RX20K2V1B1","RX25K2V1B1","RX35K2V1B1"]
["Sound pressure level","Heating","","High","dBA","47","47","48"]
["","Cooling","","High","dBA","46","46","48"]
["Standard Accessories","Drain plug","","","","1","1","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","1.55","1.55","2.09"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","0.74","0.74","1.00"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Piping connections","Level difference","IU - OU","Max.","m","12.0","12.0","12.0"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","658","658","658"]
["","","","Depth","mm","275","275","275"]
["","","","Height","mm","550","550","550"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","27","27","29"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]
["","","","","","(5) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent refrigerant piping length: 5m; level difference: 0m; indoor and outdoor unit fan speed: high.","(5) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent refrigerant piping length: 5m; level difference: 0m; indoor and outdoor unit fan speed: high.","(5) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent refrigerant piping length: 5m; level difference: 0m; indoor and outdoor unit fan speed: high."]
["","","","","","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping length: 5m; level difference: 0m; indoor and outdoor unit fan speed: high.","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping length: 5m; level difference: 0m; indoor and outdoor unit fan speed: high.","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping length: 5m; level difference: 0m; indoor and outdoor unit fan speed: high."]