{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXB-B"]
[]
[]
[]
[]
["","","","","","RXB25B5V1","RXB25B6V1","RXB25B6V19","RXB35B5V1","RXB35B6V1","RXB35B6V19","RXB50BV1B","RXB60BV1B"]
["Sound pressure level","Heating","","Nom.","dBA","","","","","","","51","51"]
["","Cooling","","Nom.","dBA","","","","","","","51","51"]
["Refrigerant","Charge","","","TCO2Eq","","","","","","","3","3"]
["","GWP","","","","","","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","","","","","","1.45","1.45"]
["","Type","","","","","","","","","","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","","","","","","","46","46"]
["","","","Min.","°CDB","","","","","","","-10","-10"]
["","Heating","Ambient","Max.","°CWB","","","","","","","18","18"]
["","","","Min.","°CWB","","","","","","","-15","-15"]
["Dimensions","Unit","","Width","mm","","","","","","","855","855"]
["","","","Depth","mm","","","","","","","328","328"]
["","","","Height","mm","","","","","","","753","753"]
["Compressor","Type","","","","","","","","","","Hermetic swing","Hermetic swing"]
["Weight","Unit","","","kg","","","","","","","44","44"]
["Power supply","Phase","","","","","","","","","","1~","1~"]
["","Frequency","","","Hz","","","","","","","50","50"]
["","Voltage","","","V","","","","","","","220-240","220-240"]
["Notes","","","","","","","","","","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","","","","","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","","","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","550","550","550","550","550","550"]
["","","","Width","mm","658","658","658","658","658","658"]
["","","","Depth","mm","275","275","275","275","275","275"]
["Weight","Unit","","","kg","27","26","26","29","28","28"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Sound pressure level","Cooling","","High","dBA","46","46","46","48","48","48"]
["","Heating","","High","dBA","47","47","47","48","48","48"]
["Refrigerant","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Charge","","","kg","0.74","0.74","0.74","1.00","1.00","1.00"]
["","Charge","","","tCO2Eq","1.5","1.5","1.5","2.1","2.1","2.1"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","15","15","15","15","15","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","12","12","12","12","12","12"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Max.","°CDB","","46","46","","46","46"]
["","Heating","Ambient","Min.","°CWB","","-15","-15","","-15","-15"]
["","","","Max.","°CWB","","18","18","","18","18"]