{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXK-A"]
[]
[]
[]
[]
["","","","","","RXK25AV1B","RXK35AV1B","RXK60AV1B","RXK50AV1B"]
["Sound pressure level","Heating","","Nom.","dBA","45","46","51"]
["","Cooling","","Nom.","dBA","45","46","51"]
["Refrigerant","Charge","","","TCO2Eq","1.5","2.1","3.0"]
["","GWP","","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","0.74","1.00","1.45"]
["","Type","","","","R-410A","R-410A","R-410A"]
["Dimensions","Unit","","Width","mm","658","658","855"]
["","","","Depth","mm","289","289","328"]
["","","","Height","mm","550","550","753"]
["Compressor","Type","","","","Hermetic swing","Hermetic swing","Hermetic swing"]
["Weight","Unit","","","kg","24","26","44"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)","(1) - All units are being tested and comply to ISO5151 (non-ducted unit) or ISO13253 (ducted unit)"]
["","","","","","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice.","(2) - All specifications are subjected to change by the manufacturer without prior notice."]
["","","","","","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases","(3) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","","","","628"]
["","","","Width","mm","","","","855"]
["","","","Depth","mm","","","","328"]
["Weight","Unit","","","kg","","","","37"]
["Compressor","Type","","","","","","","Hermetic swing"]
["Operation range","Cooling","Ambient","Min.","°CDB","","","","-10"]
["","","","Max.","°CDB","","","","46"]
["","Heating","Ambient","Min.","°CWB","","","","-15"]
["","","","Max.","°CWB","","","","18"]
["Sound pressure level","Cooling","","Nom.","dBA","","","","51"]
["","Heating","","Nom.","dBA","","","","51"]
["Refrigerant","Type","","","","","","","R-410A"]
["","Charge","","","kg","","","","1.25"]
["","Charge","","","tCO2Eq","","","","2.6"]
["","GWP","","","","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","","","","30"]
["Power supply","Phase","","","","","","","1~"]
["","Frequency","","","Hz","","","","50"]
["","Voltage","","","V","","","","220-240"]