{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLS-M"]
[]
[]
[]
[]
["","","","","","RXLS25M2V1B","RXLS35M2V1B"]
["Fan","Air flow rate","Cooling","Super low","m³/min","30.6","30.6"]
["","","Heating","Super low","m³/min","27.2","27.2"]
["","","","Super low","cfm","1080","1080"]
["","","Heating","Super low","cfm","960","960"]
["Dimensions","Unit","","Height","mm","550","550"]
["","","","Width","mm","858","858"]
["","","","Depth","mm","330","330"]
["Weight","Unit","","","kg","40","40"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Heating","Ambient","Min.","°CWB","-25","-25"]
["","","","Max.","°CWB","18","18"]
["Sound pressure level","Cooling","","High","dBA","48","48"]
["","","","Low","dBA","44","44"]
["","Heating","","High","dBA","49","49"]
["","","","Low","dBA","45","45"]
["Refrigerant","Type","","","","R-410A","R-410A"]
["","Charge","","","kg","1.3","1.3"]
["","Charge","","","tCO2Eq","2.7","2.7"]
["","GWP","","","","2087.5","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","20","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - IU","Max.","m","15","15"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V"]