{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTA-C"]
[]
[]
[]
[]
["","","","","","RXTA30C2V1B"]
["Dimensions","Unit","","Height","mm","605"]
["","","","Width","mm","930"]
["","","","Depth","mm","376"]
["Weight","Unit","","","kg","42"]
["Fan motor","Speed","Cooling","Super low","rpm","800"]
["","","Heating","Super low","rpm","400"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Heating","Ambient","Min.","°CWB","-31"]
["","","","Max.","°CWB","18"]
["Sound pressure level","Cooling","","Nom.","dBA","48"]
["","Heating","","Nom.","dBA","49.0"]
["Refrigerant","Type","","","","R-32"]
["","Charge","","","kg","0.97"]
["","Charge","","","tCO2Eq","0.66"]
["","GWP","","","","675.0"]
["Piping connections","Piping length","OU - IU","Max.","m","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","15.0"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]