{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":25,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXYTQ-TYF"]
[]
[]
[]
[]
["","","","","","RXYTQ8T7YF (Archived)","RXYTQ10T7YF (Archived)","RXYTQ12T7YF (Archived)","RXYTQ14T7YF (Archived)","RXYTQ16T7YF (Archived)","RXYTQ20TYF (Archived)","RXYTQ22TYF (Archived)","RXYTQ24TYF (Archived)","RXYTQ26TYF (Archived)","RXYTQ28TYF (Archived)","RXYTQ30TYF (Archived)","RXYTQ32TYF (Archived)","RXYTQ34TYF (Archived)","RXYTQ36TYF (Archived)","RXYTQ38TYF (Archived)","RXYTQ40TYF (Archived)","RXYTQ42TYF (Archived)","RXYTQ44TYF (Archived)","RXYTQ46TYF (Archived)","RXYTQ48TYF (Archived)"]
["Sound pressure level","Cooling","","Nom.","dBA","58 (7)","61 (7)","61 (7)","64 (7)","64 (7)"]
["Standard Accessories","Installation and operation manual","","","","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual","Installation and operation manual"]
["","Connection pipes","","","","Connection pipes","Connection pipes","Connection pipes","Connection pipes","Connection pipes"]
["Capacity range","HP","","","","8","10","12","14","16","20","22","24","26","28","30","32","34","36","38","40","42","44","46","48"]
["Operation range","Cooling","","Max.","°CDB","52","52","52","52","52"]
["","","","Min.","°CDB","-5","-5","-5","-5","-5"]
["","Heating","","Min.","°CWB","-20","-20","-20","-20","-20"]
["","","","Max.","°CWB","15.5","15.5","15.5","15.5","15.5"]
["Maximum number of connectable indoor units","","","","","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)","64 (5)"]
["Compressor","Type","","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","182","236","236","298","298"]
["Refrigerant","Charge","","","TCO2Eq","14.0","21.5","21.7","24.4","24.6"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","6.7","10.3","10.4","11.7","11.8"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["System","Outdoor unit module 2","","","","","","","","","RXYTQ12TYF","RXYTQ12TYF","RXYTQ16TYF","RXYTQ14TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ10TYF","RXYTQ12TYF","RXYTQ14TYF","RXYTQ14TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF"]
["","Outdoor unit module 3","","","","","","","","","","","","","","","","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF","RXYTQ16TYF"]
["","Outdoor unit module 1","","","","","","","","","RXYTQ8TYF","RXYTQ10TYF","RXYTQ8TYF","RXYTQ12TYF","RXYTQ12TYF","RXYTQ14TYF","RXYTQ16TYF","RXYTQ8TYF","RXYTQ8TYF","RXYTQ8TYF","RXYTQ10TYF","RXYTQ10TYF","RXYTQ12TYF","RXYTQ14TYF","RXYTQ16TYF"]
["Power input - 50Hz","Cooling","Nom.","Eurovent","kW","5.70 (19)","6.71 (19)","9.01 (19)","12.0 (19)","13.8 (19)"]
["Indoor index connection","Nom.","","","","200","250","300","350","400","500","550","600","650","700","750","800","850","900","950","1,000","1,050","1,100","1,150","1,200"]
["","Min.","","","","100","125","150","175","200","250","275","300","325","350","375","400","425","450","475","500","525","550","575","600"]
["","Max.","","","","260","325","390","455","520","650","715","780","845","910","975","1,040","1,105","1,170","1,235","1,300","1,365","1,430","1,495","1,560"]
["Cooling capacity","Nom.","","Eurovent","kW","22.4 (19)","28.0 (19)","33.5 (19)","40.0 (19)","45.0 (19)"]
["","","","Eurovent","Btu/h","76,450 (19)","95,550.0 (19)","114,350.0 (19)","136,500.0 (19)","153,550.0 (19)"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","12.7","12.7","12.7"]
["","","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","Total piping length","System","Actual","m","1,000","1,000","1,000","1,000","1,000"]
["","Gas","","OD","mm","19.1","22.2","28.6","28.6","28.6"]
["","","","Type","","Braze connection","Braze connection","Braze connection","Braze connection","Braze connection"]
["","Heat insulation","","","","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes","Both liquid and gas pipes"]
["Sound power level","Cooling","","Nom.","dBA","78 (6)","81 (6)","81 (6)","86 (6)","86 (6)"]
["Dimensions","Unit","","Width","mm","930","1,240","1,240","1,240","1,240"]
["","","","Depth","mm","765","765","765","765","765"]
["","","","Height","mm","1,685","1,685","1,685","1,685","1,685"]
["Fan","External static pressure","","Max.","Pa","78","78","78","78","78"]
["","Air flow rate","Cooling","Nom.","cfm","5,721","7,875","7,875","9,182","9,182"]
["Power supply","Phase","","","","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~","3N~"]
["","Name","","","","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1","Y1"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Voltage","","","V","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400","380-415/400"]
["Notes","","","","","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included","(1) - Cooling: T1: indoor temp. 26,7°CDB, 19,4°CWB, outdoor temp. 35°CB, AHRI 1230:2010, power input indoor units (duct type) included"]
["","","","","","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included","(2) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CB, AHRI 1230:2010, power input indoor units (duct type) included"]
["","","","","","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included","(3) - Cooling: T3: indoor temp. 29,0°CDB, 19,0°CWB, outdoor temp. 46°CB, ISO15042:2011, power input indoor units (duct type) included"]
["","","","","","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m","(4) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB, Eurovent 2015, equivalent refrigerant piping: 5m, level difference: 0m"]
["","","","","","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%).","(5) - Actual number of units depends on the indoor unit type (VRV DX indoor, etc.) and the connection ratio restriction for the system (being; 50% ≤ CR ≤ 130%)."]
["","","","","","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates.","(6) - Sound power level is an absolute value that a sound source generates."]
["","","","","","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings.","(7) - Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings."]
["","","","","","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room.","(8) - Sound values are measured in a semi-anechoic room."]
["","","","","","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual","(9) - For more details on standard accessories refer to Installation/operation manual"]
["","","","","","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(10) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current.","(11) - MSC means the maximum current during start up of the compressor. This unit uses only inverter compressors. Starting current is always ≤ max. running current."]
["","","","","","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current.","(12) - MCA must be used to select the correct field wiring size. The MCA can be regarded as the maximum running current."]
["","","","","","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(13) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - TOCA means the total value of each OC set.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(14) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - FLA means the nominal running current of the fan","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%.","(15) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions.","(16) - Soundpressure and soundpower for multi units can be calculated, following below instructions."]
["","","","","","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Maximum allowable voltage range variation between phases is 2%.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account.","(17) - Sound values are theoretical values based on sound results of individual installed units. Possible deviations due to variety of installation patterns are not taken into account."]
["","","","","","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Contains fluorinated greenhouse gases","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA","(18) - Soundpressure system [dBA] = 10*log[10^(A/10)+10^(B/10)+10^(C/10)] , with Unit A = A dBA, Unit B = B dBA, Unit C = C dBA"]
["","","","","","(19) - Cooling: Eurovent: indoor temperature: 27,0°CDB, 19,0°CWB, outdoor temperature: 35°CDB, Eurovent 2015, power input indoor units (duct type) excluded","(19) - Cooling: Eurovent: indoor temperature: 27,0°CDB, 19,0°CWB, outdoor temperature: 35°CDB, Eurovent 2015, power input indoor units (duct type) excluded","(19) - Cooling: Eurovent: indoor temperature: 27,0°CDB, 19,0°CWB, outdoor temperature: 35°CDB, Eurovent 2015, power input indoor units (duct type) excluded","(19) - Cooling: Eurovent: indoor temperature: 27,0°CDB, 19,0°CWB, outdoor temperature: 35°CDB, Eurovent 2015, power input indoor units (duct type) excluded","(19) - Cooling: Eurovent: indoor temperature: 27,0°CDB, 19,0°CWB, outdoor temperature: 35°CDB, Eurovent 2015, power input indoor units (duct type) excluded"]